

		
ENGINEERING RELEASE NOTES

Gigabit Ethernet Switch ECS4150 TIP Series
Phase 3 Firmware Version 3.12.33.263


INTRODUCTION:
[bookmark: OLE_LINK26][bookmark: OLE_LINK25][bookmark: OLE_LINK29]The ECS4150-28T is a 24*1G Base-T ports and 4*10G SFP uplink ports L2+ 1GbE Switch.
The ECS4150-28P is a 24*1G Base-T ports and 4*10G SFP uplink ports L2+ 1GbE PoE Switch.
The ECS4150-54T is a 48*1G Base-T ports and 6*25G SFP uplink ports L2+ 1GbE Switch.
The ECS4150-54P is a 48*1G Base-T ports and 6*25G SFP uplink ports L2+ 1GbE PoE Switch.
The ECS4150-28F is a 20*1G SFP ports and 4*1G Combo-RJ45-SFP ports and 4*10G SFP uplink ports L2+ 1GbE Switch.

[bookmark: OLE_LINK30]Local Console Management (LCM) allows the user to monitor and configure the ECS4150 Series from a VT-type terminal. LCM can be used to configure features such as SNMP community names and access rights, Port Enable/Disable, firmare downloads, and Device IP address as well as most other parameters. LCM can also provide statistical and diagnostic information about the entire device or an individual port.

[bookmark: OLE_LINK8]Management of the switch is password protected; the same password is used for LCM and for the Web browser interface. Prior to accessing the Management Module via a network connection, a valid IP address, subnet mask, and in some cases a default gateway must be configured using an out-of-band connection or the DHCP protocol. The management option provides SNMP, RMON (4 groups: 1,2,3,9), and Web management for system control and statistical monitoring.


	It is recommended that one thoroughly review this release notes prior to the installation or upgrade of this product.



FIRMWARE SPECIFICATION:

	Status
	Version No.
	Type
	Release Date

	[bookmark: OLE_LINK31][bookmark: OLE_LINK1]EIT0 Testing Version
	1.0.0.1
	[bookmark: OLE_LINK3][bookmark: OLE_LINK36]EIT Test Version
Gitlab: ECS4130-AC5_Phase1 Branch (2022/9/23)
	2022/9/23

	[bookmark: OLE_LINK12][bookmark: OLE_LINK13][bookmark: OLE_LINK14][bookmark: OLE_LINK15][bookmark: OLE_LINK16]EIT Testing
	1.0.0.2
	EIT Test Version
Gitlab: ECS4130-AC5_Phase1 Branch (2022/10/18)
	2022/10/18

	[bookmark: OLE_LINK2]NTC Testing
	1.0.0.3
	NTC Test Version
Gitlab: ECS4130-AC5_Phase1 Branch (2022/10/27)
	2022/10/27

	EIT Testing
	1.0.0.4
	EIT Test Version
Gitlab: ECS4130-AC5_Phase1 Branch (2022/12/01)
	2022/12/02

	NTC Testing
	1.1.0.5
	NTC Test Version
Gitlab: ECS4130-AC5_Phase1 Branch (2022/12/13)
	2022/12/13

	EIT Testing
	1.0.0.6
	EIT Test Version
Gitlab: ECS4130-AC5_Phase1 Branch (2023/01/09)
	2023/01/09

	NTC Testing
	1.1.0.7
	NTC Test Version
Gitlab: ECS4130-AC5_Phase1 Branch (2023/01/17)
	2023/01/17

	EIT Testing
	1.1.0.8
	EIT Test Version
Gitlab: ECS4130-AC5_Phase1 Branch (2023/02/07)
	2023/02/07

	NTC Testing
	1.1.0.9
	NTC Test Version
Gitlab: ECS4130-AC5_Phase1 Branch (2023/02/15)
	2023/02/15

	EIT Testing
	1.2.0.1
	EIT Test Version
Gitlab: ECS4130-AC5_Phase2 Branch (2023/03/06)
	2023/03/06

	NTC Testing
	1.2.0.2
	NTC Test Version
Gitlab: ECS4130-AC5_Phase2 Branch (2023/03/22)
	2023/03/22

	EIT Testing
	1.2.0.3
	EIT Test Version
Gitlab: ECS4130-AC5_Phase2 Branch (2023/04/20)
	2023/04/20

	NTC Testing
	1.2.0.4
	NTC Test Version
Gitlab: ECS4130-AC5_Phase2 Branch (2023/04/27)
	2023/04/27

	EIT Testing
	1.2.0.5
	EIT Test Version
Gitlab: ECS4130-AC5_Phase2 Branch (2023/05/18)
	2023/05/18

	NTC Testing
	1.2.0.6
	NTC Test Version
Gitlab: ECS4130-AC5_Phase2 Branch (2023/05/26)
	2023/05/26

	EIT Testing
	1.3.0.1
	EIT Test Version
Gitlab: ECS4130-AC5_Phase3 Branch (2023/07/20)
	2023/07/20

	NTC Testing
	1.3.0.2
	NTC Test Version
Gitlab: ECS4130-AC5_Phase3 Branch (2023/08/08)
	2023/08/08

	EIT Testing
	1.3.0.3
	EIT Test Version
Gitlab: ECS4130-AC5_Phase3 Branch (2023/09/08)
	2023/09/08

	NTC Testing
	1.3.0.4
	NTC Test Version
Gitlab: ECS4130-AC5_Phase3 Branch (2023/09/20)
	2023/09/20

	EIT Testing
	1.3.0.6
	EIT Test Version
Gitlab: ECS4130-AC5_Phase3 Branch (2023/09/25)
	2023/09/25

	NTC Testing
	1.3.0.7
	NTC Test Version
Gitlab: ECS4130-AC5_Phase3 Branch (2023/10/18)
	2023/10/18

	NTC Testing
	1.3.0.8
	NTC Test Version
Gitlab: ECS4130-AC5_Phase3 Branch (2023/10/26)
	2023/10/26

	EIT Testing
	3.2.0.234
	EIT Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2023/11/10)
	2023/11/10

	NTC Testing
	3.2.1.234
	NTC Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2023/12/25)
	2023/12/25

	NTC Testing
	3.2.2.241
	NTC Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2024/01/16)
	2024/01/16

	EIT Testing
	3.2.3.241
	EIT Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2024/01/23)
	2024/01/23

	EIT Testing
	3.2.4.241
	EIT Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2024/01/31)
	2024/01/31

	EIT Testing
	3.2.5.241
	EIT Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2024/02/29)
	2024/02/29

	EIT Testing
	3.2.6.243
	EIT Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2024/08/05)
	2024/08/05

	EIT Testing
	3.2.7.243
	EIT Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2024/08/08)
	2024/08/08

	EIT Testing
	3.2.8.254
	EIT Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2025/12/04)
	2025/12/04

	NTC Testing
	3.2.9.254
	NTC Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2025/12/12)
	2025/12/12

	EIT Testing
	3.2.10.261
	EIT Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2026/01/05)
	2026/01/05

	EIT Testing
	3.2.11.261
	EIT Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2026/01/07)
	2026/01/07

	NTC Testing
	3.2.12.261
	EIT/NTC Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2026/01/16)
	2026/01/16

	EIT/NTC Testing
	3.2.13.261
	EIT/NTC Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2026/01/26)
	2026/01/26

	EIT/NTC Testing
	3.2.14.261
	EIT/NTC Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2026/02/06)
	2026/02/06

	EIT Testing
	3.2.17.261
	EIT/NTC Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2026/03/04)
	2026/03/04

	EIT/NTC Testing
	3.2.18.261
	EIT/NTC Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2026/03/24)
	2026/03/24

	EIT(QA) Testing
	3.2.19.262
	EIT/QA Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2026/04/24)
	2026/04/24

	EIT(QA) Testing
	3.12.22.262
	EIT/QA Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2026/05/25)
	2026/05/25

	EIT(QA) Testing
	3.12.26.262
	EIT/QA Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2026/06/15)
	2026/06/15

	NTC Testing
	3.12.30.263
	NTC Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2026/07/24)
	2026/07/24

	EIT(QA) Testing
	3.12.31.263
	EIT/QA Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2026/08/05)
	2026/08/05

	EIT(QA) Testing
	3.12.32.263
	EIT/QA Test Version
Gitlab: BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8 Branch (2026/08/11)
	2026/08/11


LOADER:

	Status
	Version No.
	Type
	Release Date

	Test Version
	0.0.0.4
	Gitlab: ECS4130-AC5_Phase1 Branch (2022/9/23)
	2022/9/23

	Test Version
	0.0.0.6
	Gitlab: ECS4130-AC5_Phase1 Branch (2022/10/18)
	2022/10/18

	Test Version
	0.0.0.7
	Gitlab: ECS4130-AC5_Phase1 Branch (2022/12/01)
	2022/12/02

	NTC Testing
	0.0.0.8
	NTC Test Version
Gitlab: ECS4130-AC5_Phase1 Branch (2022/12/13)
	2022/12/13

	Test Version
	0.0.0.9
	Gitlab: ECS4130-AC5_Phase1 Branch (2023/01/09)
	2023/01/09

	Test Version
	0.0.1.0
	Gitlab: ECS4130-AC5_Phase2 Branch (2023/03/06)
	2023/03/06

	Test Version
	0.0.1.1
	Gitlab: ECS4130-AC5_Phase2 Branch (2023/04/20)
	2023/04/20

	Test Version
	0.0.1.2
	Gitlab: ECS4130-AC5_Phase2 Branch (2023/05/18)
	2023/05/18

	Test Version
	0.0.1.5
	Gitlab: ECS4130-AC5_Phase3 Branch (2023/07/20)
	2023/07/20

	Test Version
	0.0.1.6
	Gitlab: ECS4130-AC5_Phase3 Branch (2023/08/08)
	2023/08/08

	Test Version
	0.0.1.8
	Gitlab: ECS4130-AC5_Phase3 Branch (2023/09/08)
	2023/09/08



HARDWARE COMPATIBILITY:	

ALL


BOOTPROM COMPATIBILITY:

ALL


NETWORK MANAGEMENT SOFTWARE SUPPORT:

	NMS Platform
	Version No.
	Module No.

	TBD
	 
	 



If you install this image, you may not have control of all of the latest features of this product until the next version(s) of network management software. Please review the software release notes for your specific network management platform for details.


SUPPORTED FUNCTIONALITY:

Please see the AC5-AC5X-Aldrin2_FeatureSpec_20230905.xlsx

INSTALLATION AND CONFIGURATION NOTES:

[bookmark: OLE_LINK34][bookmark: OLE_LINK33]In general, the ECS4150 Series Switch will be shipped to you pre-configured with this version of firmware. If you would like to upgrade an existing ECS4150 Series Switch, please follow the TFTP download instructions that are included with your firmware image upgrade kit.
 
FIRMWARE CHANGES AND ENHANCEMENTS:

The following Known Issues have been fixed in this release of firmware.

Runtime V1.0.0.1, Loader V0.0.0.4
	1
	NA
	



Runtime V1.0.0.2, Loader V0.0.0.6
	1
	ECS4150EC-13
	SFP port can not send and receive packets

	2
	ECS4650EC-2
	Synchronize the modification of ECS4150 to ECS4650, add ECS4650 related macro definitions to solve compilation errors

	3
	ECS4150EC-5
	Delete Diag partition and resize Ecos partition

	4
	ECS4650EC-2
	Fix the problem of build user and upgrade u-boot version

	5
	ECS4150EC-29
	TrafficSeg/VLAN-ProtocolBased:Segmentation Fault

	6
	ECS4150EC-32
	mac-address-table aging time in range cannot be set

	7
	ECS4150EC-20
	Fix add/delete static route

	8
	ECS4150EC-33
	PortSecurity-0180.rspan up-link on port failed

	9
	ECS4150EC-5
	Modify the upgrade detection mechanism in u-boot

	10
	ECS4150EC-50
	ipv6 nd ra suppress:Segmentation Fault

	11
	ECS4150EC-13
	adapt MMU and flowcontrol of ECS4150

	12
	ECS4150EC-51
	IPV6 RA MTU not work

	13
	ECS4150EC-51
	IPV6 RA not send packet

	14
	ECS4150EC-35
	Unnecessary print when type Traceroute

	15
	ECS4150EC_5
	Fix the problem of recovery image signature verification failed

	16
	ECS4650EC-2
	Port-mapping for ac5x

	17
	ECS4150EC-28
	interface vlan 1 didnot init and cannot be created after copy startup-config running-config

	18
	ECS4150EC-20
	Save the static route and restart DUT, staticd proc crash.

	19
	ECS4150EC-61
	flow control andd shutdown port not work well after save config/reload



Runtime V1.0.0.3, Loader V0.0.0.6
	1
	None
	add submodule cpss4.3.8

	2
	None
	upgrade sdk to 4.3.8 for ac5x

	3
	None
	Optimize the compilation of openssl

	4
	None
	adapt cpss4.3.8 for ECS4150

	5
	ECS4150EC-71
	Modify simba displayed system name for EC new model name

	6
	None
	add linux-4.14.76_CnM-22.03.0.patch for sdk 4.3.8

	7
	ECS4150EC-74
	modify OID of ecs4650-ac5x to make snmp can work correctly

	8
	ECS4150EC-75
	segmentation fault when no ipv6 neighbor



Runtime V1.0.0.4, Loader V0.0.0.7
	1
	ECS4150EC-70
	snmp-host with version 1 did't receive warm start trap.

	2
	ECS4150EC-79
	Remove the CLI command: Loopback detection mode

	3
	ECS4150EC-1
	adapt board id 1 for PoE device

	4
	ECS4150EC-74
	modify OID of ecs4650-ac5x to make snmp can work correctly.

	5
	None
	Add c99 cflags for 4130_ac5 and 4650_ac5x

	6
	ECS4150EC-79
	Remove the CLI command: Loopback detection mode

	7
	ECS4150ECX_8
	Set I2C to no channel switching mode

	8
	ECS4150ECX-14
	The trap of "copy running-config file" will cause segmentation fault.

	9
	None
	Support RIP on FRR

	10
	ECS4150EC-80
	when ZTP can not resolve ip address, it keeps printing error message.

	11
	ECS4150EC-92
	kernel oops some times when calling kfree_skb

	12
	ECS4650EC_8
	Add i2c device driver for AC5X

	13
	ECS4150EC-95
	Web: Ports arrangement in WebUI is different from front panel of the device.

	14
	ECS4150EC-101
	WEB: DUT does not support option 82 information in web Help page.

	15
	ECS4150EC-83
	SFP: Got "DEV_SWDRV_SetPortInterfaceMode(): Line = 15729 , error_id=7" when SFP is removed or set to "media-type sfp-forced 10gsfp.

	16
	ECS4150EC-71
	Modify simba displayed system name for EC new model name

	17
	ECS4650EC_8
	Pass the nand partition parameters in u-boot to the kernel

	18
	ECS4650EC_8
	Upgrade loader version

	19
	ECS4150EC-100
	Support dhcp relay option display

	20
	ECS4150EC-105
	Configuration:Copy running configuration with name "Factory_Default_Config.cfg" to tftp server. DUT return error and rebooting itself.

	21
	None
	Add CLI Command about smart-part

	22
	ECS4650EC-10
	adapt ACL for AC5X

	23
	ECS4150EC-107
	DHCPv6 Relay: add restrictions for relay destination

	24
	ECS4150EC-103
	DUT does not reject invalid DHCP Relay address setting, and it cannot relay Request packets.

	25
	ECS4150EC-109
	DHCPv6 Relay: After we delete and add DHCPv6 Relay, DUT cannot send out DHCPv6 RelayForw to Server.

	26
	ECS4150EC-98
	The DUT will crash and reboot with watchdog when configure the seletct qinq on LACP port.

	27
	ECS4150EC-123
	Crash and watchdog reboot after set reload at "3/7/2023"(DD/MM/YYYY) and "7:3"(HH:MM) and then apply the setting from web.

	28
	ECS4150EC-120
	There is no "FTPS Upload" and "FTPS Download" when it is changed from "HTTP Upload"

	29
	ECS4650EC-15
	Add CLI Command about smart-part

	30
	ECS4150EC-116
	The DUT will pop "Segmentation Fault!" and reboot when create and delete the sample-rate of sflow

	31
	ECS4150EC-114
	WEB: Failed to link to DHCP-SNP and DHCP-SNPv6 help page.

	32
	ECS4150EC-129
	Cluster: The SNMP trap relayed by commander always be coldstart trap

	33
	ECS4150EC-121
	Support SCP on WEB GUI File copy

	34
	ECS4150EC-91
	ARP: The DUT will pop error message when change the suspend VLAN to active VLAN

	35
	ECS4150EC-115
	IPv6-FTP:It's failed to copy http-certificate via IPv6 FTP.

	36
	ECS4150EC-132
	ImageDownload:Got debug message "Set not check Image Version" when set it from back door.

	37
	ECS4150EC-117
	Fix the wrong range of transceiver-threshold

	38
	ECS4150EC-119
	Solve some bug about the htm txt of WebHelp

	39
	ECS4150EC-76
	POE function implementation.

	40
	ECS4150EC-84
	1000 SFP will packet loss and get error counter

	41
	ECS4150EC-5
	Port POE i2c pin


Runtime V1.1.0.5, Loader V0.0.0.8
	1
	ECS4150EC-81
	Static ARP not recover when link up

	2
	ECS4150EC-99
	Support BOOTP on AC5

	3
	ECS4150EC-118
	MSTP: The DUT will freezes and reboot automatically when config the mst instance of MSTP.

	4
	ECS4150EC-138
	"show hosts" Cli command output can't seprate to different page

	5
	ECS4650EC-4
	Distinguish between build FRR of ECS4150 and ecs4650

	6
	ECS4650EC-14
	1.all traps will become warmstart trap. 2.ac5x frr build will report error

	7
	ECS4150EC-71
	Modify the certificate displayed system name

	8
	ECS4150EC-76
	POE function implementation

	9
	ECS4150EC-76
	POE function implementation

	10
	ECS4150EC-5
	Fix the issue of http upload failure  port type

	11
	ECS4150EC-76
	POE function implementation.

	12
	ECS4650EC-18
	fdb entry write fail for daQosIndex is 1

	13
	ECS4650EC_5
	Fix the issue of alarm led status wrong

	14
	ECS4650EC_5
	Add cpld upgrade tools

	15
	ECS4650EC_5
	Adds fan control functionality



Runtime V1.1.0.6, Loader V0.0.0.9
	1
	ECS4650EC-16
	QINQ]It will report error message when type command "dot1q-tunnel system-tunnel-control"

	2
	ECS4650EC-19
	[MVR6]support

	3
	ECS4150EC-152
	Ipv6 route configures can not be deleted

	4
	ECS4150EC-156
	[snmp]:snmp walk will report error messages.

	5
	ECS4150EC_5
	Adds fan control functionality

	6
	ECS4150EC-4
	Support FRR BGP

	7
	ECS4150EC-71
	Modify simba displayed system name for EC new model name

	8
	ECS4150EC-166
	POE:Used power of the ports don't reset to 0 when disable POE function

	9
	ECS4650EC-10
	adapt port negotiation and init error of ECS4650EC

	10
	ECS4650EC-20
	SCP not support on WEB GU

	11
	ECS4150EC-170
	ConfigFileMgmt: Got "% Memory is not enough" & "Failed to copy running configuration to local" when read/write flash at the same time.

	12
	ECS4150EC-180
	ImageDownload: Run "http upload" from WebUI and "reload" from CLI at the same time, reload shall be rejected.

	13
	ECS4150EC-171
	[mib]:Get all sub-object of lldpconfiguration, it can not get any response.

	14
	ECS4150EC-166
	POE:Used power of the ports don't reset to 0 when disable POE function

	15
	ECS4150EC-176
	System: Watchdog reboot after http_upload V1.0.0.3 (2nd opcode) into flash

	16
	ECS4150EC-151
	Got big counters after clear counters.

	17
	ECS4150EC-168
	Model name is wrong in PoE help page

	18
	ECS4150EC-158
	POE software version showing Version 0x00(Hex)error and changing power budget from 364w to 370w

	19
	ECS4650EC-13
	VLAN, AMTR function verication

	20
	ECS4650EC-13
	VLAN, AMTR function verication

	21
	ECS4150EC-187
	POE:Do not show "Version is WRONG" error message and add "SRAM programming have been completed" message

	22
	ECS4150EC-189
	[mib]:ifOutDiscards is empty.

	23
	ECS4650EC-25
	Can not trap ARP packets to CPU

	24
	ECS4650EC-13
	VLAN, AMTR function verication(Fix protocol VLAN on SNMP)

	25
	ECS4150EC-174
	system: ports 27&28 will down when unplug the cables from dynamic trunk(port 25&26)

	26
	ECS4150EC-194
	POE and NonPOE check during boot up

	27
	ECS4650EC_5
	Fix the gpio configuration and disable interrupt

	28
	ECS130AC5_104
	Fix the issue of sfp link down and link up automatically

	29
	ECS4150EC-194
	POE and NonPOE check during boot up

	30
	ECS4150EC_104
	Mask and clear interrupts

	31
	ECS4150EC-193
	Segmentation Fault happened after be the cluster member

	32
	ECS4150EC-5
	Add force full speed cmd

	33
	ECS4150EC-167
	POE maximum allocation is useless

	34
	ECS4150EC-183
	MIB:Value of igmpSnoopPortClearStatistics is always 0

	35
	ECS4150EC-157
	[xSTP] The DUT crashed when setting the mst port-priority config

	36
	ECS4150EC-4
	L3 Feature Verification

	37
	ECS4150EC-160
	DDM: Special value of transceiver-threshold shall be rejected

	38
	ECS4150EC-4
	L3 Feature Verification

	39
	ECS4150EC-183
	MIB:Value of igmpSnoopPortClearStatistics is always 0.

	40
	ECS4150EC-84
	1000 SFP will packet loss and get error counter

	41
	ECS4150EC-84
	1000 SFP will packet loss and get error counter

	42
	ECS4150EC-181
	MIB: Display of igmp profile range is wrong.

	43
	ECS4150EC-169
	PoE: DUT cannot send LLDP with Power Via MDI TLV.

	44
	ECS4150EC-190
	MLD: Content of ipv6 mld profile cannot be showed when use "show ipv6 mld profile".

	45
	ECS4150EC-185
	MIB: mvrVlanStatisticsTable (1.3.6.1.4.1.259.10.1.55.1.44.33) is not necessary.



Runtime V1.1.0.7, Loader V0.0.0.9
	1
	ECS4150EC-183
	MIB:Value of igmpSnoopPortClearStatistics is always 0.

	2
	ECS4150EC-5
	Adapt to poe led control function

	3
	ECS4650EC-8
	Fix AC5X build error

	4
	ECS4150EC-161
	POE maximum priority is useless

	5
	ECS4150EC-200
	SNMP:The mib browser will show timeout when walk the dot1xAuthSessionUsername(9) of OID.

	6
	ECS4150EC-195
	Mirror-ACL: Failed to add ACL mirroring because "DEV_SWDRV_SetDestPortForMacMirror(): Line = 11859 , error_id=-1, arg = 3,1,1,1"

	7
	ECS4150EC-173
	Web: WebUI without action doesn't return to login page after 300 seconds



Runtime V1.1.0.8, Loader V0.0.0.9
	1
	ECS4150EC-161
	PoE: Port number priority is useless.

	2
	ECS4150EC-173
	Web: WebUI without action doesn't return to login page after 300 seconds.

	3
	ECS4150EC-164
	Fix the problem that the poe button does not respond

	4
	ECS4150EC-177
	system:got giant counter after clear counters or shutdown/no shutdown ports

	5
	ECS4150EC-204
	The web help page is incorrect

	6
	ECS4650EC-4
	Support BGP SNMP

	7
	ECS4150EC-211
	Modify the CPU code and queue for some ACL trapped packets

	8
	ECS4150EC-207 & ECS4150EC-208
	LLDP: dot3-tlv poe cannot be disabled.
LLDP: There is no command to enable/disable lldp med-tlv ext-poe. 

	9
	ECS4150EC-177
	system:got giant counter after clear counters or shutdown/no shutdown ports

	10
	ECS4150EC-87
	Internal Loopback: Internal loopback test is failed on sfp port

	11
	ECS4150EC-206
	WEB: model name in portsStatus menu is disappear

	12
	ECS4150EC-184
	MVR: Clear mvr statistics of one port would clear mvr statistics of all ports.

	13
	ECS4150EC-203
	mib:Source IP address is wrong in MAC ACL.

	14
	ECS4150EC-160
	DDM: Special value of transceiver-threshold shall be rejected

	15
	ECS4150EC-212
	Fix the problem that the port 28 led light green when port 1 link up

	16
	ECS4150EC-205
	Web: There is no "Auto Mode" checkbox and selection for "Interface > Port > Transceiver"

	17
	ECS4150EC-213
	WebUI Version is different from CLI

	18
	ECS4150EC-209
	DUT can not provide power class 1,2,4 to PD

	19
	ECS4150EC-201
	IPv6-AddrConfig:DUT sends a lot of NS and NA.

	20
	ECS4150EC-186
	MLAG:The traffic will loas half flow a few minutes or more when shutdown the port-channel 1 of 3rd.

	21
	ECS4150EC-201
	IPv6-AddrConfig:DUT sends a lot of NS and NA.

	22
	ECS4150EC-186
	MLAG:The traffic will loas half flow a few minutes or more when shutdown the port-channel 1 of 3rd.



Runtime V1.1.0.9, Loader V0.0.0.9
	1
	ECS4150EC-5
	Fix the problem that the accton driver install failed

	2
	ECS4150EC-229
	statistics-0161 0290:clear counters port not clear counters

	3
	ECS4150EC-226
	Modify model name & image name

	4
	ECS4150EC-226
	Modify model name & image name

	5
	ECS4150EC-226
	Modify model name & image name

	6
	ECS4150EC-226
	Modify model name & image name

	7
	ECS4150EC-226
	Modify model name & image name

	8
	ECS4150EC-218
	DAI for IPSG whitelist not work



Runtime V1.2.0.1, Loader V0.0.1.0
	1
	ECS4650EC-5
	Fix route forwarding source mac replace and support BGP SNMP

	2
	ECS4150EC-216
	Adapt MMU,media_type for AC5X

	3
	ECS4150EC-235
	DHCP-SNP: Disable and enable DHCP-SNP option 82, DUT cannot forward DHCP Request packets to trust Port.

	4
	ECS4130EC-215
	Adapt to rx los, tx fault ,dying gasp interrupt

	5
	ECS4130EC-243
	Voice VLAN: DUT does not reject invalid OUI setting with zero address.

	6
	ECS4150EC-241
	LLDP: After we reset this lldp notify interval from maximum field value, DUT cannot send out notify trap message.

	7
	ECS4130EC-215
	Adapt fan speed adjustment

	8
	ECS4650EC-7
	Support OSPF on FRR

	9
	ECS4150EC-216
	Adapt qos and diffserv for AC5X

	10
	ECS4150EC-219
	Phase2 L3 feature verification

	11
	ECS4150EC-233
	AC5X POE implementation

	12
	ECS4130EC-211
	Modify the CPU code and queue for some ACL trapped packets

	13
	ECS4130EC-215
	Adapt sfp led control

	14
	ECS4150EC-217
	temporarily fix the problem about "port mirror" of AC5X

	15
	ECS4150EC-245
	Some processes crash when receive double vlan packets

	16
	ECS4130EC-242
	^ Point to the wrong problem

	17
	None
	Fix show running-cfg maxinum-paths

	18
	ECS4650EC-7
	Support OSPF on FRR

	19
	ECS4130EC-215
	Adapt for LED control and fan control

	20
	ECS4130EC-215
	Adapt for interrupts control and acc cmd on loader

	21
	ECS4130EC-215
	Upgrade loader version

	22
	ECS4150EC-211
	Modify ARP and LLDP queue

	23
	ECS4150EC-248
	AC5X bt port can't open and close properly

	24
	ECS4150EC-216
	Adapt polarity of sfp port and add fec command for AC5X

	25
	ECS4150EC-217
	fix the problem about "vlan mirror/mac mirror/acl mirror" of AC5X

	26
	ECS4150EC-226
	phase1&phase2:Modify model name & image name



Runtime V1.2.0.2, Loader V0.0.1.0
	1
	ECS4150EC-250
	ipv6 link-local ip is active when the system is boot up

	2
	ECS4150EC-216
	Adapt flow control for AC5X

	3
	ECS4130EC_215
	Adapt for cpld upgrade

	4
	ECS4150EC-239
	Statistic: Input error packets to Port; the Discard and Error packets count are incorrect.

	5
	ECS4150EC-251
	AC5X ACL:bind acl to port out failed

	6
	ECS4150EC-281
	Diffserv-1090: packets can not be forwarded when packets match QOS policy setting

	7
	ECS4150EC-262
	AC5X and AC5 not unify with stormctrl max setting.

	8
	ECS4150EC-263
	AC5X Statistics-0050:count twice as send with bad crc packets.

	9
	ECS4150EC-274
	Fix request irq fail when restoring default

	10
	ECS4150EC-238
	After disable and enable poe port. maximum allocation can work properly

	11
	ECS4150EC-233
	Optimize POE code

	12
	ECS4650EC-7
	Support OSPF on FRR

	13
	ECS4650EC-7
	Support OSPF on FRR

	14
	ECS4150EC-252
	AC5X L2SW-0160 0170:Speed-duplex display incorrect when auto negotiation.

	15
	ECS4150EC-217
	apply "sflow sampling" of AC5X



Runtime V1.2.0.3, Loader V0.0.1.1
	1
	ECS4150EC-254
	Support IEEE 802.1ag (CFM) & Y.1731 (Ethernet OAM)

	2
	ECS4150EC-230
	Phase3(ECS4150-28F-I) Port bring-up and mapping

	3
	ECS4130EC-215
	Repair port 49 and port 50 rx los detection

	4
	ECS4150EC-266
	AC5X VoiceVlan:voice vlan priority not be set

	5
	ECS4150EC-230
	Phase3(ECS4150-28F-I) Port bring-up and mapping(SDK segmentation fault)

	6
	ECS4150EC-255
	AC5X L2SW: no negotiation cannot be set.

	7
	ECS4150EC-254
	Support IEEE 802.1ag (CFM) & Y.1731 (Ethernet OAM)

	8
	ECS4150EC-254
	Support IEEE 802.1ag (CFM) & Y.1731 (Ethernet OAM)

	9
	ECS4130EC-215
	modify usb reg for hardward test

	10
	ECS4150EC-230
	Phase3(ECS4150-28F-I) Port bring-up and mapping(For AC5X compile error)

	11
	ECS4150EC-295
	DHCP-Server: CLI can't stop printing dhcp binding information when connect more than 256 DHCP client.

	12
	ECS4150EC-266
	AC5X VoiceVlan:voice vlan priority not be set

	13
	ECS4150EC-273
	AC5X ratelimit output not same as AC5.

	14
	ECS4150EC-295
	DHCP-Server: CLI can't stop printing dhcp binding information when connect more than 256 DHCP client.

	15
	ECS4150EC-233
	maximum power 730w can not provide for 24 port 30w.

	16
	ECS4150EC-298
	WebUI: The number of ports is wrong in front panel.

	17
	ECS4150EC-210
	When insert and remove PD very quickly , the led will on even no PD on this port.

	18
	ECS4150EC-307
	Help_Page: Please remove ECMP help page

	19
	ECS4150EC-308
	DHCP Relay: DUT does not reject to set itself as relay server address.

	20
	ECS4650EC-10
	Fiber port can not up when insert SFP.

	21
	ECS4150EC-311
	vlanTraslationPortTable mib get return partial result.

	22
	ECS4150EC-310
	802.1X-Supplicant: The supplicat port can join the port-channle member.

	23
	ECS4150EC-313
	MIB: Get the MIB object dhcpv6DynamicProvisionStatus, this response value is incorrect.

	24
	ECS4650EC-8
	Fan control developement for both 54P and 54t

	25
	ECS4150EC-297
	HTTPs: Transfer certificate is error and shown memory not enough from web browser

	26
	ECS4150EC-315
	DHCPv6 Relay: After we save running and reload this DUT; it lose dhcpv6 relay setting.

	27
	ECS4150EC-309
	PoE: Model name and maximum power are wrong in help page.

	28
	ECS4650EC-8
	Adaptation of driver & peripheral device & PoE

	29
	ECS4650EC-10
	Remove speed 100half/10half cli cmd and modify the description of stormcontrol.

	30
	ECS4650EC-7
	Support OSPF on FRR

	31
	ECS4650EC-21
	Support vrrp on AC5X

	32
	ECS4150EC-322
	ImageMgmt: Warning message and log status is inconsistent

	33
	ECS4150EC-319
	WebUI: Web can't return to login page after DUT reboots.

	34
	ECS4150EC-230
	Phase3(ECS4150-28F-I) Port bring-up and mapping(For AC5X compile error)

	35
	ECS4150EC-319
	WebUI: Web can't return to login page after DUT reboots.

	36
	ECS4150EC-217
	conflict about sflow-sampling and port mirror

	37
	ECS4150EC-303
	Some invalid or reserve IPV6 address can be accepted

	38
	ECS4150EC-304
	SelectiveQinQ: CVID set from SNMP can exceed range (1-4094).

	39
	ECS4150EC-317
	LLDP: There are four mistakes on lldp help page.

	40
	ECS4150EC-230
	Phase3(ECS4150-28F-I) Port bring-up and mapping(For AC5 max trunk group number)

	41
	ECS4150EC-327
	Syslog: There is no log history after "copy sftp file".

	42
	ECS4150EC-215
	Upgrade CPSS SDK to 4.3.10

	43
	ECS4150EC-324
	ImageMgmt: Reload machine is wrong (It's also occurred at ECS4130)

	44
	ECS4650EC-7
	Support OSPF on FRR

	45
	ECS4150EC-217
	conflict about sflow-sampling and port mirror

	46
	ECS4650EC-21
	Fix vrrp crash on ac5

	47
	ECS4150EC-329
	MLAG: The traffic will packets loss when reboot the DUT.

	48
	None
	update uboot version

	49
	ECS4150EC-334
	DNS: The number of host entry are not sequenceal

	50
	ECS4650EC-10
	When shutdown/no shutdown the mlag member, the syncd mac may syncd to incorrect port.

	51
	ECS4150EC-331
	Traffic Segmentation configuration is not save when eth port 1/27.28 is in uplink or downlink port list

	52
	ECS4150EC-333
	command "ip http authentication aaa exec-authorization" won't be show in running-config

	53
	ECS4150EC-215
	driver & peripheral device adaptation

	54
	ECS4150EC-318
	MSTP: The port-channel will disappear on instance 0 of MSTP

	55
	ECS4150EC-300
	Adapt to Cable-diagnostics function

	56
	ECS4150EC-330
	Watchdog: Reboot after segment fault.

	57
	ECS4130EC-284
	delate igmp snooping



Runtime V1.2.0.4, Loader V0.0.1.1
	1
	ECS4150EC-320
	SystemMgmt: Temperature of rising/falling alarm is different with spec and system no shutdown when temperature is over 76 degrees.

	2
	ECS4150EC-305
	SelectiveQinQ: CLI has no commands to show the configuration for port-channel individually.

	3
	ECS4130EC-264
	Failed to set ratelimit output.

	4
	ECS4650EC-8
	Assign correct fan speed according to the board_id

	5
	ECS4650EC-22
	Support IGMP/PIM on FRR

	6
	ECS4650EC-22
	Fix IGMP/PIM compile

	7
	ECS4150EC-1
	Modify environment in Linux shell

	8
	ECS4150EC-319
	Web can't return to login page after DUT reboots

	9
	ECS4150EC-265
	simba stacking

	10
	ECS4150EC-234
	Internal Loopback: All 1G ports are down after run "test loop internal interface interface ethernet 1/X".

	11
	ECS4650EC-21
	Fix bug of vrrp

	12
	ECS4150EC-325
	Watchdog: Trigger watchdog reboot because "cat: can't open '/proc/1470/ustack': No such file or directory"

	13
	ECS4150EC-353
	VoiceVlan-0411:voicevlan didnot tranmit dscp value well

	14
	ECS4150EC-339
	Trap： The DUT cannot send out the "tcnTrap(63)" when cause the topology change

	15
	ECS4150EC-352
	Fix cable diag causing problems with port link status

	16
	ECS4150EC-312
	WebUI:Mirror display is different on port/vlan/mac-address

	17
	ECS4150EC-356
	Add ecCloud management daemon (mgmtd) on ECS4150 series switches.

	18
	ECS4150EC-300
	Adapt to Cable-diagnostics function for ECS4650_AC5



Runtime V1.2.0.5, Loader V0.0.1.2
	1
	ECS4150EC-215
	Fix cable diag causing problems with build error

	2
	None
	Add show ip igmp interface command

	3
	ECS4150EC-325
	Watchdog: Trigger watchdog reboot because "cat: can't open '/proc/1470/ustack': No such file or directory"

	4
	ECS4650EC-8
	ECS4650_AC5X POE development

	5
	ECS4650EC-13
	VLAN, AMTR function verification(Fix protocol VLAN on stacking)

	6
	ECS4150EC-365
	ecCloud agent (mgmtd) cannot resolve DNS for registration service.

	7
	ECS4150EC-367
	HelpPage: Default value of some DoS Protection items in help page is enabled

	8
	ECS4150EC-303
	Some invalid or reserve IPV6 address can be accepted

	9
	ECS4150EC-360
	Voice VLAN: DUT does not reject set itself MAC as OUI MAC

	10
	ECS4650EC-8
	ECS4650_AC5X POE development

	11
	ECS4150EC-368
	Test loopback: Got "Internal loopback test: faied" when it's not joined VLAN 1

	12
	ECS4650EC-8
	ECS4650_AC5X POE development

	13
	ECS4650EC-8
	ECS4650_AC5X POE development

	14
	ECS4650EC-8
	adjust macro range; modify defination of board type

	15
	ECS4150EC-363
	System Test: After we set DHCP-SNP VLAN to suspended; DUT return error, ping session timeout and all unicast data looping

	16
	ECS4150EC-370
	Implement SNMP ipCidrRoute

	17
	None
	Fix zebra compilation

	18
	ECS4650EC-12
	XSTP.VLAN translation.QinQ.LBD.UDLD function verication

	19
	None
	fix poedrv complie error

	20
	None
	Fix snmp compilation

	21
	ECS4150EC-299
	Test loopback: implement loopback function for fiber port.

	22
	ECS4150EC-374
	SNMP:When DUT reject PC login to DUT by mgmt-ip-filter setting, it send out unknown trap

	23
	ECS4650AC5X-7
	Support OSPF on FRR

	24
	ECS4150EC-362
	System Test: Shutdown and no shutdown LACP trunk for overnight, DUT reload itself.

	25
	ECS4150EC-380
	Fix cable diag test failed with running a second test while the first test is not completed

	26
	ECS4650EC-19
	MVR6 SUPPORT

	27
	ECS4150EC-378
	ImageMgmt: SFTP function does not work

	28
	None
	Init SNMP long variate and fix some parameter check failures

	29
	ECS4150EC-378
	ImageMgmt: SFTP function does not work

	30
	ECS4150EC-377
	Rate-limit: Rate-limit output rate is not accurate.

	31
	ECS4150EC-375
	Watchdog: Reboot after "Segmentation Fault!" (/usr/bin/l2_l4_proc)

	32
	ECS4150EC-265
	simba ac5x stacking

	33
	ECS4150EC-384
	3MS#20131128 WHT: ECS4150P-28 missing suboption port-description in ip dhcp snooping information option remote-id string“ command

	34
	ECS4150EC-265
	simba ac5x stacking packets transfer

	35
	ECS4150EC-265
	simba ac5x stacking packets transfer

	36
	ECS4650EC-8
	ECS4650_AC5X POE development

	37
	None
	Fixed the slave device cpu cannot send packets

	38
	ECS4150EC-383
	Add sfp-forced ifmode CLI command for 25G and 10G fiber port.

	39
	ECS4150EC-265
	simba ac5x stacking packets transfer

	40
	ECS4650EC-8
	ECS4650_AC5X POE development

	41
	ECS4150EC-369
	Fix port link status detect error

	42
	ECS4150EC-369
	Fix port link status detect error

	43
	ECS4150EC-383
	Modify the default value of ifmode to sr_lr.

	44
	ECS4150EC-215
	Fix the problem that i2c operation is not locked

	45
	None
	Fix the issue of eth2 failure



Runtime V1.2.0.6, Loader V0.0.1.2
	1
	ECS4150EC-230
	Phase3(ECS4150-28F-I) Port bring-up and mapping(Adjust combo port)

	2
	ECS4150EC-216
	simba ac5x copper port can not linkup in init port manager state

	3
	ECS4650EC-32
	Support UDPhelper Feature

	4
	ECS4650EC-8
	ECS4650_AC5X POE development

	5
	ECS4650EC-8
	ECS4650_AC5X POE development

	6
	ECS4150EC-376
	COMB_MSTPt: The CPU Utilization of ECS4150-54T/P is 22%, but the ECS4150-28T/P is only 4% of CPU Utilization.

	7
	ECS4650EC-30
	Voice VLAN,OAM,LLDP Feature Verification

	8
	ECS4150EC-328
	Fix the problem that Power-saving does not work for ECS4150-54P (No any action)

	9
	ECS4150EC-350
	Unicast input/output is not enough when line speed 5 minutes.

	10
	ECS4650EC-20
	Some features do not work on stacking mode

	11
	ECS4650EC-8
	ECS4650_AC5X POE development

	12
	ECS4650EC-9
	Standalone & Stackable: SNMP, WEB, Download/Upgrade,L2MCAST Feature Verification

	13
	ECS4150EC-394
	LACP: The 25G of LACP that can not work



Runtime V1.3.0.1, Loader V0.0.1.5
	1
	ECS4650EC-30
	Voice VLAN,OAM,LLDP Feature Verification

	2
	ECS4650EC-20
	Packet filtering of L2 control CDP/PVST  Feature Verification

	3
	ECS4150EC-354
	L2SW:not pause packets receive when flowcontrol enabled.

	4
	ECS4650EC-30
	Voice VLAN,OAM,LLDP Feature Verification

	5
	ECS4650EC-31
	L3 verification based on stack

	6
	ECS4650EC-31
	L3 verification based on stack

	7
	ECS4150EC-312
	WebUI:Mirror display is different on port/vlan/mac-address

	8
	ECS4150EC-402
	RSTP: The default cost is incorrect on 25G link port.

	9
	ECS4650EC-34
	change the switch stacking port option range from 1-2 to 1-3

	10
	ECS4150EC-405
	MVR: SNMP walk can't get correct group table after join and leave some groups.

	11
	ECS4150EC-404
	MVR: Show mvr statistics input counter includes unused VLAN data.

	12
	ECS4150EC-403
	When group has no members, up time of this group is not empty.

	13
	ECS4650EC-20
	DHCPv6 relay fails when one vlan in the multi-destination has no ipv6 globle address

	14
	ECS4150AT-5
	L2sw:capability show with symmetric when it should not be shown

	15
	ECS4150EC-402
	RSTP: The default cost is incorrect on 25G link port.  (remove the define AC5 AC5X)

	16
	ECS4650EC-29
	Enhancement for 2G DDR, compatible with 1G DDR

	17
	ECS4650EC-29
	Fix the problem that ECS4650AC5X build error

	18
	ECS4150AT-9
	Igmpsnooping-0030 0430 0660 0850 0870 0950 1060 1710 1860:igmp query didnot work after saveconfig and reboot s1,set igmp enable

	19
	ECS4650EC-13
	VLAN, AMTR function verification(fix traffic segmentation on stacking)

	20
	ECS4150EC-383
	XCVR-Cable-IOT: Port will be down after moved the cable when it's connected by ET7302-DAC-3M(M5)

	21
	ECS4150AT-3
	MVR.DUT down when set mvr domain 1 type source

	22
	ECS4650EC-20
	MSTP-1150 : DUT no response when Set DUT1 and DUT2 mst name

	23
	ECS4650EC-20
	system up time over 496 days will reset

	24
	ECS4150AT-13
	Reboot the DUT that will pop debug message

	25
	ECS4650EC-26
	simba ac5x stacking support 8 devices

	26
	ECS4650EC-30
	Voice VLAN,OAM,LLDP Feature Verification

	27
	ECS4650EC-8
	POE function not work on ECS4650_AC5X with 2G DDR

	28
	ECS4650EC-20
	DHCP relay option82 snmp update

	29
	ECS4650EC-35
	show destination uplink ethernet value  is different from setting

	30
	ECS4650EC-39
	show switch stacking interfaces brief error when switch don't set switch stacking button

	31
	ECS4150AT-9
	Igmpsnooping-0030 0430 0660 0850 0870 0950 1060 1710 1860:igmp query didnot work after saveconfig and reboot s1,set igmp enable

	32
	ECS4650EC-29
	Add cmd for upload the image of nand

	33
	ECS4650EC-29
	Adapt for cpld upgrade and show version

	34
	ECS4650EC-22
	Support IGMP/PIM on FRR

	35
	ECS4650EC-30
	Voice VLAN,OAM,LLDP Feature Verification

	36
	ECS4150EC-383
	Add ifmode CLI command for ecs4650_ac5x.

	37
	ECS4650EC-9
	Standalone & Stackable: SNMP, WEB, Download/Upgrade,L2MCAST Feature Verification

	38
	ECS4650EC-10
	After add the ifmode cli command, stacking can not work normally.

	39
	ECS4650EC-13
	VLAN, AMTR function verification(fix subnet/mac vlan rule setting)

	40
	ECS4650EC-26
	when setting stacking-port option to 1, stacking can not be established successfully.

	41
	ECS4650EC-8
	POE stacking slave LED function and monitoring power do not work.

	42
	ECS4650EC-40
	add fec CLI command and add option 25gsfp of CLI command media-type sfp-forced for ecs4650_ac5x

	43
	ECS4650EC-29
	Sync the code of sfp led and Cable-diag

	44
	ECS4650EC-13
	VLAN, AMTR function verification(fix traffic segmentation on stacking)

	45
	ECS4650EC-40
	CLI command fec rs being reset by CLI command media-type sfp-forced 25gsfp

	46
	ECS4650EC-8
	Sync DEV_SWDRV_BOARD_Init from ecs4130_ac5 for Fan function

	47
	ECS4650EC-10
	(MLAG)For stacking, if the non mlag member is the port of slave , the mac learned on non mlag member can not syncd to peer.

	48
	ECS4150EC-407
	DHCP SNP: DUT send out unknown remote-id value as set maximum description string.

	49
	ECS4650EC-40
	After add the fec cli command, stacking can not work normally.

	50
	ECS4650EC-12
	XSTP，VLAN translation，QinQ，LBD，UDLD function verication

	51
	ECS4650EC-7
	Support OSPF on FRR

	52
	ECS4650EC-7
	Support OSPF on FRR

	53
	ECS4650EC-9
	Standalone & Stackable: SNMP, WEB, Download/Upgrade,L2MCAST Feature Verification

	54
	ECS4650EC-9
	Standalone & Stackable: SNMP, WEB, Download/Upgrade,L2MCAST Feature Verification

	55
	ECS4150EC-1
	update the guidelines of making manufactory bin file

	56
	ECS4150EC-408
	DHCP Relay: Client failed to get Reply as it send unicast Request to DUT sometimes.

	57
	ECS4150AT-17
	Igmpsnooping-1060: general query suppression not work well after saveconfig&reboot

	58
	ECS4650EC-47
	Modify the image name for sw release

	59
	ECS4150AT-17
	Igmpsnooping-1060: general query suppression not work well after saveconfig&reboot

	60
	ECS4150EC-293
	Support MVR6

	61
	ECS4650EC-43
	Create PBE of eps5520 & eps5720 for muxi customization

	62
	ECS4650EC-7
	Support OSPF on FRR

	63
	ECS4650EC-7
	Support OSPF on FRR

	64
	ECS4150EC-408
	DHCP Relay: Client failed to get Reply as it send unicast Request to DUT sometimes.

	65
	ECS4650EC-7
	Support OSPF on FRR

	66
	ECS4650EC-9
	Standalone & Stackable: SNMP, WEB, Download/Upgrade,L2MCAST Feature Verification

	67
	ECS4650EC-60
	Upgrade FRR 8.5.2 version

	68
	ECS4150EC-416
	Add library to parse env of u-boot

	69
	ECS4150EC-416
	Partition suitable for simba to parse env

	70
	ECS4150EC-416
	Set the baud rate when switching the startup

	71
	ECSS4650EC-8
	Adaptation of driver & peripheral device & PoE

	72
	ECS4650EC-7
	Support OSPF on FRR

	73
	ECS4150EC-416
	Add ignore file for libubootenv and yaml

	74
	ECS4650EC-7
	Support OSPF on FRR

	75
	ECS4650EC-57
	ATC:atc trap display unit 2 port 1 info with 57, recommand to display with unit/port.

	76
	ECS4150EC-416
	Fix the problem of build failed for libubootenv and yaml

	77
	ECS4650EC-44
	Stacking: Master and Slave would swap after save reloading

	78
	ECS4650EC-7
	Support OSPF on FRR

	79
	ECS4650EC-7
	Support OSPF on FRR

	80
	ECS4650EC-7
	Support OSPF on FRR

	81
	ECS4650EC-7
	Support OSPF on FRR

	82
	ECS4650EC-7
	remove virtual-link commands

	83
	ECS4650EC-53
	MAC-Filter-0050: network-access mod mac-authentication can be enable when port enable gust vlan

	84
	ECS4650EC-71
	AMTR-0050:mac-address table delete after aging time with start time as first learned.

	85
	ECS4650EC-79
	Support RFC 2933(IGMP SNMP)

	86
	ECS4650EC-71
	AMTR-0050:mac-address table delete after aging time with start time as first learned.

	87
	ECS4650EC-77
	BGP distance is NOT effective

	88
	ECS4650EC-7
	Support OSPF on FRR

	89
	ECS4650EC-75
	BGP Resdistribution OSPF is NOT effective

	90
	ECS4650EC-57
	Port on slave can not genarate temerature high alarm/warning.

	91
	ECS4650EC-8
	Adaptation of driver & peripheral device & PoE

	92
	ECS4650EC-7
	Support OSPF on FRR

	93
	ECS4650EC-61
	the master's stacking-port option corresponding phyport on the slave is not present

	94
	ECS4150IT-9
	adding the filtering feature to CLI commands of show running, show log ram and show log flash

	95
	ECS4650EC-87
	BGP-Accesslist[stacking]：network would missing

	96
	ECS4650EC-86
	BGP-1610 neighbor 192.168.1.253 timers connect 0 failed

	97
	ECS4650EC-8
	Adaptation of driver & peripheral device & PoE

	98
	ECS4650EC-94
	Migration packaging scripts and image upgrade

	99
	ECS4650EC-8
	Light off the stack LED during the startup process.

	100
	ECS4650EC-82
	BGP-0720/1490: show ip bgp prefix-list is wrong

	101
	ECS4650EC-8
	Implement POE stacking led function.Push button function.

	102
	ECS4650EC-100
	The authentication key of OSPF is wrong in show running

	103
	ECS4650EC-98
	Failed to set the ip OSPF priority.

	104
	ECS4650EC-99
	DUT1 should reject this setting router-id 0.0.0.0

	105
	ECS4650EC-106
	show arp error

	106
	ECS4650EC-7
	Support OSPF on FRR

	107
	ECS4150IT-9
	adding the filtering feature to CLI commands of show running, show log ram and show log flash

	108
	ECS4650EC-8
	Implement POE stacking function.

	109
	ECS4650EC-88
	sh ip bgp community-list needs all list

	110
	ECS4650EC-7
	Support OSPF on FRR

	111
	None
	modify ECS4150.mib and ECS4650.mib

	112
	ECS4650EC-7
	Support OSPF on FRR

	113
	ECS4650EC-26
	Stacking: default stacking-port option set to 2.

	114
	ECS4650EC-8
	In stacking mode,remove stacking line to become standalone and RJ45 led keep lighting.

	115
	ECS4650EC-7
	Support OSPF on FRR

	116
	ECS4650EC-75
	BGP Resdistribution OSPF is NOT effective

	117
	ECS4650EC-8
	Build ecs4130_ac5 error

	118
	ECS4150IT-11
	Modify that after sending and receiving a specific ERROR packet, it is also recorded in the "Error Input" part of the "show interface counter"

	119
	ECS4150it-9
	Standalone & Stackable: adding the filtering feature to cli commands of show running, show log ram and show log flash

	120
	ECS4150EC-419
	Update cpld upload shell for 28F-I



Runtime V1.3.0.2, Loader V0.0.1.6
	1
	ECS4150EC-411
	Fix the display problem of Cable Diag test results

	2
	ECS4650EC-107
	Support SNMP/WEB PIM

	3
	ECS4650EC-67
	Diffserve-1140-1190: Policy Map PHB Input not work well

	4
	ECS4150IT-11
	Modify that after sending and receiving a specific ERROR packet, it is also recorded in the "Error Input" part of the "show interface counter".

	5
	ECS4150EC-420
	Shutdown/No Shutdown[ECS4150-28F]:The port(Opto-electronic) is recovered too slowly after no shutdown

	6
	ECS4650EC-121
	CFM [stacking]: After we change maximum mep_id, it cannot send out all mep CCMs.

	7
	ECS4650EC-125
	CFM [stacking]: DUT still send out LBM as delete down-mep under loopback test.

	8
	ECS4650EC-86
	RMON:show rmon statistics only displays unit 1 intrefaces,unit 2 interfaces didnot be displayed

	9
	ECS4650EC-137
	SNTP: DUT can't accepted sntp server hostname

	10
	ECS4150EC-419
	When combo port's media-type is copper-forced or VAL_portComboForcedMode_sfpPreferredAuto and not insert SFP, it still diaplay 1000SFP.

	11
	ECS4650EC-143
	Signature verification error when u-boot loads diag

	12
	ECS4650EC-130
	WEB: Loss CFM Help page

	13
	ECS4650EC-130
	WEB: Loss CFM Help page

	14
	ECS4150IT-9
	adding the filtering feature to CLI commands of show running, show log ram and show log flash

	15
	ECS4150IT-9
	adding the filtering feature to CLI commands of show running, show log ram and show log flash

	16
	ECS4650EC-129
	PIM [stacking]: The downstream router cannot receive all multicast packets

	17
	ECS4650EC-151
	BGP: The DUT will pop message when added the neighbor with maximum number of remote-as.

	18
	ECS4650EC-142
	IGMP[Stacking]: Max Resp Time in queries is wrong when change igmp max-resp-interval.

	19
	ECS4650EC-153
	LLDP-MED: CLI doesn't provide command to enable or disable MED ext-poe TLV.

	20
	ECS4650EC-139
	IGMP[Stacking]: DUT sends igmpv3 query and report when igmp version is 2.

	21
	ECS4650EC-141
	ECMP: DUT cannot forward all ipv6 ecmp route traffic

	22
	ECS4650EC-129
	PIM [stacking]: The downstream router cannot receive all multicast packets

	23
	ECS4650EC-155
	MVR6: CLI has no show debug mvr6 command.

	24
	ECS4650EC-116
	CLI shows debug messages when click Add/Show button of UDP Helper Address via WebUI.

	25
	ECS4150EC-434
	Voicevlan-0340[ECS4150-28F]:port leave voice vlan after port down/up

	26
	ECS4650EC-156
	VRRP: Cannot modify the priority of vrrp

	27
	ECS4650EC-167
	CFM [stacking]: After we interrupt loopback test by manual, DUT still send out LBM.

	28
	ECS4650EC-148
	MVR6:Dynamic mrouter port can not be created when mvr6 source port receives tagged mld query

	29
	ECS4150IT-16
	NTP Client show ntp status error

	30
	ECS4650EC-173
	OSPF [stacking]: After we configure routing timers, system halted and rebooting.

	31
	ECS4150IT-3
	exclude VLAN

	32
	ECS4650EC-159
	TWAMP: Count field value in Server Greeting packet is wrong.

	33
	ECS4650EC-160
	TWAMP: Typesetting is wrong when Sender or Reflector address is long IPv6 address.

	34
	ECS4650EC-185
	CPU-Guard[Stacking]: Current Threshold becomes 1000 packets/sec when enable and disable CPU guard.

	35
	ECS4150IT-3
	exclude VLAN

	36
	ECS4150IT-3
	exclude VLAN

	37
	ECS4650EC-128
	IGMP:cli show debug messages when input multicast data

	38
	None
	Add submodule of cpss_4.3.11

	39
	None
	Adapt to cpss 4.3.11

	40
	ECS4650EC-134
	IGMP[Stacking]: Behavior is wrong when change robustval and query-interval value.

	41
	ECS4150EC-438
	Fix the problem that TX DISABLE causes usb not to work normally

	42
	ECS4650EC-162
	PIM: DUT still forward multicast data to downstream even entry status is Null.

	43
	ECS4650EC-202
	IGMP: Dynamic groups doesn't be restricted.

	44
	ECS4650EC-202
	IGMP: Dynamic groups doesn't be restricted.

	45
	ECS4650EC-181
	BGP: The DUT does not rejected the setting when exceed the maximum peer-group.

	46
	ECS4650EC-95
	When there is a loopback link between master and slave devices, it will print "ISC_PacketIncoming:receive invalid ISC packet"

	47
	ECS4650EC-145
	WEB: Loss Routing Protocal Help page.

	48
	ECS4650EC-61
	the master's stacking-port option corresponding phyport on the slave is not present

	49
	ECS4650EC-197
	MVR6_Web: Priority is not in global setting

	50
	ECS4650EC-168
	BGP: Delete the route-map rule, show the route-map that does not empty.

	51
	ECS4650EC-191
	MVR6:802.1p Forwarding priority is useless

	52
	ECS4150EC-432
	L2SW-0270[ECS4150-28F]:port cannot up when disable auto negotiation.

	53
	ECS4650EC-200
	MVR6: Different domain can set the same vlan.

	54
	ECS4150EC-444
	After configuring pppoe intermediate-agent port-format-type remote-id in a port, the user failed to delete it in no-form

	55
	ECS4150EC-436
	Fix the problem that get baudrate form config file causes system crash

	56
	ECS4650EC-171
	POE slave device version is wrong when stacking using "show power mainpower"

	57
	ECS4650-23
	support cli filtering

	58
	ECS4650EC-192
	RIP: Learning the 81881 entries of route that does not keep on the route entiers

	59
	ECS4650EC-200
	MVR6: Different domain can set the same vlan.

	60
	ECS4650EC-212
	BGP: The DUT will pop error message and the DUT will freeze.

	61
	ECS4650EC-61
	the master's stacking-port option corresponding phyport on the slave is not present(Adapt AC5)

	62
	ECS4150EC-441
	Fan speed regulation strategy adapted to ECS4130-28F



Runtime V1.3.0.3, Loader V0.0.1.8
	1
	ECS4150EC-488
	CLONE - [GVRP-PDU-0600, GVRP-PDU-0660] Attribute value verification fail

	2
	ECS4150EC-483
	[IPv6-SNMP-0020, SNMP-0020] Some specifications of snmp are no longer applicable because of adding mgmtd

	3
	ECS4150EC-471
	MVR6: Behavior is wrong when groups exist and the source port with mrouter port receives one general query.

	4
	ECS4150EC-470
	MVR6: Non-MVR6 group multicast data received from the receiver port cannot be forwarded by MLDSNP.

	5
	ECS4150EC-469
	MVR6: Normal ports cannot register groups that belong to mvr6 profile.

	6
	ECS4150EC-468
	MVR6: Group is wrong when show mvr6 statistics output/input.

	7
	ECS4150EC-467
	The LED of Port 25 and 27 cannot light up.

	8
	ECS4150EC-466
	MVR6_Web: Port role in MVR6 Memver List is wrong when source port mode is dynamic.

	9
	ECS4150EC-465
	MVR6: MIB doesn't support MVR6.

	10
	ECS4150EC-464
	MVR6: Source IP address of queries sent out from receiver port is wrong when source port receives queries.

	11
	ECS4150EC-463
	MVR6: DUT sends report messages to all source ports even mldsnp mrouter port exists.

	12
	ECS4150EC-462
	MVR6: MVR6 doesn't support mldv2 report messages.

	13
	ECS4150EC-461
	MVR6: MLD queries received from the source port would be forwarded to another source and receiver ports.

	14
	ECS4150EC-460
	MVR6: MLD queries received from the receiver port would be forwarded to another receiver and normal ports.

	15
	ECS4150EC-459
	Web_Help: Help of L3 function shall be removed and MVR6 help shall be added.

	16
	ECS4150EC-457
	DHCP Relay: DUT relay double DHCP Request frames to Server.

	17
	ECS4150EC-456
	MIB: Not support to get/set exclude-vlan by MIB.

	18
	ECS4150EC-455
	Exclude-vlan: Change the bit-mask setting, DUT cannot forward vlan traffic correctly.

	19
	ECS4150EC-453
	Dynamic Provision: After we save bootfile and reload this DUT; DUT is halted and reload itseld.

	20
	ECS4150EC-451
	(ECS4150-28F-I)Web File: The Source File Name always display "-1"

	21
	ECS4150EC-450
	WebUI: We can't copy public key via webUI.

	22
	ECS4150EC-449
	lease remove command since 4150-28F not support 25G SFP.

	23
	ECS4150EC-448
	PPPoE: Web can set the circuit-id and remote-id to HAN001Z001/I1 atm 01/05:1.3, but the CLI will reject.

	24
	ECS4150EC-447
	Enhance command of "show running-config key-words"

	25
	ECS4150EC-411
	CableDiag: SFP port is not supported. But it's displayed NT.



Runtime V1.3.0.4, Loader V0.0.1.8
	1
	ECS4150EC-511
	[4150-28F][802.1ag-CFM-0370]: the "defRemoteCCM" condition can not be cleared

	2
	ECS4150EC-510
	[4150-28F][802.1ag-CFM-0320]: DUT still transmit AIS packet when it received CCM

	3
	ECS4150EC-509
	StormCtrl: Got "Failed to set broadcast storm on port 1" when it's set "switchport multicast packet-rate 25600" on channel member.

	4
	ECS4150EC-447
	Enhance command of "show running-config key-words"

	5
	ECS4150EC-513
	The certificate in the https web page is incorrect



Runtime V1.3.0.6, Loader V0.0.1.8
	1
	ECS4150EC-474
	CLONE - Hyperoptic 需求(ECS4150/Simba)



Runtime V1.3.0.7 Loader V0.0.1.8
	1
	ECS4150EC-527
	[ECS4150-28F][1QVLAN-1790]: the infomation of vlan member port is not correct when we save adn reboot DUT

	2
	ECS4150EC-523
	GVRP[ECS4150-54T]: DUT down after set GVRP function

	3
	ECS4150EC-522
	MVR6: Query of Output Statistics of port interface can not count.

	4
	ECS4150EC-521
	The MEP field in the 'show erps instance' information is displayed as Err

	5
	ECS4150EC-520
	CableDiag: Combo port shall not be displayed "NS" by default.

	6
	ECS4150EC-519
	Systemboot: Got strange message when reboot on ECS4150-54T/54P.

	7
	ECS4150EC-518
	Config file name max size cause default config after reboot.

	8
	ECS4150EC-517
	Media-type: 1000SFP could not be communicated when 28Fv2-I and 54T/54P.

	9
	ECS4150EC-500
	DDM: Warning/alarm is only generated at 1st time

	10
	ECS4150EC-464
	MVR6: Source IP address of queries sent out from receiver port is wrong when source port receives queries.

	11
	ECS4150EC-459
	Web_Help: Help of L3 function shall be removed and MVR6 help shall be added.

	12
	ECS4150EC-214
	DDM: Warning/Alarm will not be generated after re-insert SFP.



Runtime V1.3.0.8 Loader V0.0.1.8
	1
	ECS4150EC-534
	MVR/MVR6: G Query counter of MVLAN increases when receiver ports send the general query.

	2
	ECS4150EC-530
	System: After we configure DUT; it show exception and system halted.

	3
	ECS4150EC-529
	L3 DHCP Relay: After we enable and disable relay option82, DUT cannot forward DHCP packets.

	4
	ECS4150EC-528
	WEB: Please remove CFM mep monitor display and description in WEB and Help.

	5
	ECS4150EC-503
	MVR6: Groups cannot be removed when DUT receives done reports after join and leave groups 12 hours continuously.



Runtime V3.2.0.234 Loader V0.0.1.8
	1
	ECS4150TIP-104
	Create a new PBE(project_build_environment) for ECS4150-TIP Phase3

	2
	ECS4150TIP-107
	Phase3 [CLI] add command to update and show ucentral certificate

	3
	ECS4150TIP-106
	Porting function profile related modifications to ecs4150 phase3 branch

	4
	ECS4150TIP-105
	ECS4150TIP Phase 3 development：
    1. Porting function profile on BR_ECS4150TIP_Phase3_BaseOn_ECS4150_V1.3.0.8.
    2. Create CLI command about display license.
    3. Support to update inverse-vector image.
    4. Add option about "update image without checking function profile" in backdoor.
    5. Add bypass function in common code.

	5
	ECS4150TIP-110
	Phase3 porting ucentral client

	6
	ECS4150TIP-109
	[ECS4150TIP Phase3] Change the default authenticate to root/openwifi.



Runtime V3.2.1.234 Loader V0.0.1.8
	1
	ECS4150TIP-112
	[ECS4150-28P-TIP] set speed to 10000 error when configuring SFP port by cloud sdk



Runtime V3.2.2.241 Loader V0.0.1.8
	1
	ECS4150TIP-117
	Add CLI command to enable/disable ucentral debug message and display OLS version

	2
	ECS4150TIP-118
	Remove unnecssary function for license in fs.



Runtime V3.2.3.241 Loader V0.0.1.8
	1
	ECS4150TIP-119
	upgrade OLS to V1.2



Runtime V3.2.4.241 Loader V0.0.1.8
	1
	ECS4150TIP-120
	upgrade ECS4150, ucentral OLS version to V1.2_4107d36c



Runtime V3.2.5.241 Loader V0.0.1.8
	1
	ECS4150TIP-121
	upgrade OLS to V1.3



Runtime V3.2.6.243 Loader V0.0.1.8
	1
	ECS4150TIP-131
	[PoE] The maximum power allocation settings are different from CLI and SNMP MIB

	2
	ECS4150TIP-128
	Command "power inline maximum allocation" cannot be saved on port interface.

	3
	ECS4150TIP-127
	Command "power inline maximum allocation" cannot be disabled.

	4
	ECS4150TIP-126
	Enhancement logging command

	5
	ECS4150TIP-125
	[PoE] The maximum power allocation settings are different from CLI and WEB

	6
	ECS4150EC-582
	Port LED will be blinking abnormally.
	Port LED will be blinking abnormally.



Runtime V3.2.7.243 Loader V0.0.1.8
	1
	ECS4150TIP-134
	Update ucentral-client v1.3.5 for ECS4150



Runtime V3.2.8.254 Loader V0.0.1.8
	1
	ECS4150TIP-132
	IGMP general query cannot counters in "sh ip igmp snooping statistics query vlan 1", but actually it's keep sending IGMP query pkts.

	2
	ECS4150TIP_137
	Record all client option information to a file

	3
	ECS4150TIP-142
	upgrade OLS to 3.2.4rc5

	4
	ECS4150TIP-146
	porting security issue into 4150-tip branch

	5
	ECS4150TIP-148
	disable runtime backdoor ¡BLinux shell backdoor and "__super" username & password.

	6
	ECS4150TIP-151
	Security issue：udp socket 5151 bind to local address（127.0.0.1）

	7
	ECS4150TIP-152
	PoE issue on ECS4150 TIP version.

	8
	ECS4150TIP-154
	Enhancement suport SHA256 Algorithm for encryption

	9
	ECS4150TIP-155
	After we add and delete some static routes, it cannot create maximum 32 routes on DUT.

	10
	ECS4150TIP-157
	Enhancement: Save the output of "show tech_support" and copy log on to flash

	11
	ECS4150TIP-158
	Modify the default value of "ip dhcp client class-id" to OpenLAN

	12
	ECS4150TIP-159
	DHCP : Add vender class identifier in parameter request list(option 55).

	13
	ECS4150TIP-161
	Update ucentral client to 3.2.10

	14
	ECS4150TIP-171
	NTP: The DUT will freezing and reboot when added and delete the ntp server more times.(TIP)

	15
	ECS4150TIP-173
	need to get ntp servers from dhcp offer reply option 42, please help to add dhcp discover request for option 42

	16
	ECS4150TIP-175
	It's stuck for 5 minutes while doing show running config with specific configure

	17
	ECS4150TIP-172
	Cable diagnostics is reporting cable length as positive on some ports when no cable is connected

	18
	ECS4150TIP-177
	customer want to low down the fan speed because the noise.

	19
	ECS4150TIP-178
	The way to reset configuration or password without super password.

	20
	ECS4150TIP-179
	Support DHCP option 138 and 224

	21
	ECS4150TIP-180
	TCP port 2601 will be scanned as open port via NMAP.

	22
	ECS4150TIP-181
	Update ucentral ols 4.1 & Improve ucentral redirector/certificate command

	23
	ECS4150TIP-208
	Support display and delete ec_pki certificates

	24
	ECS4150TIP-209
	Reduced packagded firmware size

	25
	ECS4150TIP-194
	Support interfaces feature for ucentral rest api；Increase cgi buffer to 128k for large json data.

	26
	ECS4150TIP-192
	Support ucentral rest ethernet

	27
	ECS4150TIP-193
	support ucentral rest switch

	28
	ECS4150TIP-199
	free buffer after json_dumps

	29
	ECS4150TIP-212
	The multicast IP packets with destination 224.0.0.251 will be discarded on ECS4150.

	30
	ECS4150TIP-211
	Configurable ucentral client log print out to console

	31
	ECS4150TIP-195
	Add error message for services

	32
	ECS4150TIP-213
	Ucentral restAPI: etherent ACL get duplicate result

	33
	ECS4150TIP-215
	Allow REST API requests from loopback address




Runtime V3.2.9.254 Loader V0.0.1.8
	1
	ECS4150TIP-210
	Added copy image or configuration RestFul API.

	2
	ECS4150TIP-221
	Ucentral restAPI: support GET with JSON body filter for ethernet and switch

	3
	ECS4150TIP-222
	Ucentral restAPI: physical device, set port rate-limit 0 failed

	4
	ECS4150TIP-200
	Implement the RESTful API security mechanism

	5
	ECS4150TIP-220
	Services: support to get method with body

	6
	ECS4150TIP-223
	Ucentral restAPI: support GET with JSON body filter for inerfaces.

	7
	ECS4150TIP-224
	Unit: Support to get method with body.

	8
	ECS4150TIP-225
	Ucentral restAPI: ethernet voice vlan mode "manual" does not work

	9
	ECS4150TIP-227
	Ucentral restAPI: ACL rule ethertype should be HEX string

	10
	ECS4150TIP-230
	Update ucentral to ols 4.1 restfulapi



MODIFICATIONS:

Runtime V3.2.10.261 Loader V0.0.1.8
	1
	ECS4150TIP-289
	Error Handler：DAI IPv4-RemotePing IPv4-SourceGuard

	2
	ECS4150TIP-285
	Error Handler  RADIUS-Acct SSHv2

	3
	ECS4150TIP-290
	Error Handler：LLDP MLAG MSTP STP LACP PortTrunk

	4
	ECS4150TIP-283
	Error Handler：ACL Diffserv

	5
	ECS4150TIP-286
	Error Handler：DHCP-Snooping NTP SYSLOG Console-Telnet DNS mDNS HTTP DHCP

	6
	ECS4150TIP-270
	UcentralRESTAPI: The default gateway cannot be configured via the uCentral REST API.

	7
	ECS4150TIP-264
	RD backdoor cannot work well

	8
	ECS4150TIP-288
	it cannot setup mlag doman id over 1000

	9
	ECS4150TIP-293
	[Rest API] Add trunk member to ethernet port list

	10
	ECS4150TIP-294
	get json config is different after setup port trunk

	11
	ECS4150TIP-292
	[Rest API] MAC ACL ignores cos when matched pkt type is untag

	12
	ECS4150TIP-287
	[Rest API] MVR: The source and receiver ports cannot be set at the same time.

	13
	ECS4150TIP-214
	Without backdoor - Remove runtime backdoor 、Linux backdoor and super account&MD5 Checksum File Generation

	14
	ECS4150TIP-228
	[ACL-Compress-0010-0190] It has Capability "EXCLUDED_VLAN" on ACL rule.

	15
	ECS4150TIP-280
	[Rest API][VLAN] Create invalid VLAN id by rest API will return 200 OK and delete other exist VLAN.

	16
	ECS4150TIP-276
	[Rest API] set media-type sfp-forced for SFP port in port-speed setting

	17
	ECS4150TIP-278
	After setting "ip domain-lookup" in CLI, the Restful API cannot retrieve data.

	18
	ECS4150TIP-269
	[Rest API] IPv6-AddrConfig: The result is different when put ipv6 addressing "dynamic".

	19
	ECS4150TIP-275
	[Rest API] MVR: One profile can not associate multiple domain via Rest API.

	20
	ECS4150TIP-266
	[Rest API] IGMPSNP: The value is incorrect when the 'Last Member Query Interval' is set via the REST API.

	21
	ECS4150TIP-272
	[Rest API] switch port-isolation supports range interfaces

	22
	ECS4150TIP-274
	RESTAPI: The DUT crashes with a segmentation fault and reboots when an invalid Ethernet port range is provided.

	23
	ECS4150TIP-263
	[Rest API] correct some filed name error

	24
	ECS4150TIP-250
	UcentralRESTAPI: Remove the local-server field and add an enable/disable option for the NTP client

	25
	ECS4150TIP-253
	[Rest API] ACL: It does not support the source and destination port options of the IPv6 extended ACL.

	26
	ECS4150TIP-261
	Added Unit String verification mechanism.

	27
	ECS4150TIP-239
	UcentralRESTAPI: If authentication-mode is sent as empty, it will be set to force-unauthorized.

	28
	ECS4150TIP-240
	[Rest API] VLAN: DUT not reject to create VLAN name over maximum string.

	29
	ECS4150TIP-260
	[Rest API] IP Source Guard: Configure binding entry with invalid settingy restAPI; DUT accept it and display incorrect result in running configuration.

	30
	ECS4150TIP-241
	[Rest API] ACL: '?' can be set to an ACL name using the restAPI.

	31
	ECS4150TIP-242
	[Rest API] DHCP-SNP: Configure remote-id over 64 characters; it display invalid string in running configuration.

	32
	ECS4150TIP-243
	[Rest API] DHCP-SNP: Configure circuit-id over 32 characters; it display invalid string in running configuration.

	33
	ECS4150TIP-245
	[Rest API] Voice VLAN: DUT not reject OUI MAC with invalid format; and it display invalid OUI MAC in running configuration.

	34
	ECS4150TIP-246
	[Rest API] Voice vlan: Configure OUI description over 30 characters; it not return error and display invalid string in running configuration.

	35
	ECS4150TIP-247
	[Rest API] IP ARP inspection: Configure rate-limit over 750 by restAPI; it not return error and display incorrect setting in running configuration.

	36
	ECS4150TIP-251
	[Rest API] DHCP-SNP: Configure rate-limit with invalid setting by restAPI; DUT not reject this setting.

	37
	ECS4150TIP-252
	[Rest API] LLDP: Configure all global parameter setting with invalid setting value by restAPI; it not reject it and return any error message.

	38
	ECS4150TIP-254
	[Rest API] IP ARP inspection: Configure lldp-med-location-civic-device-type with invalid setting by restAPI; it not reject setting and return error message.

	39
	ECS4150TIP-255
	[Rest API] Voice VLAN: Configure voice vlan priority with invalid setting by restAPI; it not reject this setting and return error message.

	40
	ECS4150TIP-257
	[Rest API] STP: Configure all global parameter setting with invalid setting value by restAPI; it not reject it and return any error message.

	41
	ECS4150TIP-258
	[Rest API] STP: Configure auto recovery-interval with invalid setting value by restAPI; DUT not reject it and return any error message.

	42
	ECS4150TIP-249
	Ucentral restAPI: support select ports range config for igmpsnp static-mcast-groups

	43
	ECS4150TIP-248
	enhancement：SSH/Console: limit number of login attempts

	44
	ECS4150TIP-237
	[Rest API] select-ports with range style of ethernet

	45
	ECS4150TIP-235
	Ucentral restAPI: support select ports range config for inerfaces.

	46
	ECS4150TIP-232
	Services: select ports support range config

	47
	ECS4150TIP-236
	[Rest API] IP Source Guard: Failed to put the max-acl-boinding and MAC binding entry.

	48
	ECS4150TIP-234
	[Rest API] VLAN: Join Trunk to VLAN; DUT return error.

	49
	ECS4150TIP-231
	ECS4150-TIP Mlag support static LACP function

	50
	ECS4150TIP-291
	[ECS4150-54P resuful API] :it will cause "Segmentation Fault" after input port1 rate-limit "25000000"

	51
	ECS4150TIP-279
	[Rest API] MVR: 400 Bad Request is displayed when set the trunk to receiver port.

	52
	ECS4150TIP-277
	[Rest API] MVR: The profiles cannot be removed via Rest API.

	53
	ECS4150TIP-273
	[Rest API] MVR: The DUT responds with a 200 OK when the value is set outside the range.

	54
	ECS4150TIP-271
	[Rest API] Voice VLAN: DUT not reject OUI MAC and mask over length by RestAPI; and it display different OUI MAC in running configuration.

	55
	ECS4150TIP-268
	After setting the port monitor mac-address in CLI, the Restful API cannot retrieve this value.

	56
	ECS4150TIP-265
	[Rest API] IP ARP inspection: Configure vlan-acl-rule with non-existing ACL name by restAPI; it not reject setting and write different ACL rule to running.




Runtime V3.2.11.261 Loader V0.0.1.8
	1
	ECS4150TIP-298
	[LACP-0050~0480] LACP cannot auto binding on the port-channel

	2
	ECS4150TIP-297
	[RADIUS-Acct-0030~0480] Error message prompt when set/remove radius server host configuration.

	3
	ECS4150TIP-296
	[Rest API] workaround when ucentral binds ACL before creating ACL

	4
	ECS4150TIP-284
	Error Handler：VoiceVLAN




Runtime V3.2.12.261 Loader V0.0.1.8  OLS 4.2.0rc1
	1
	ECS4150TIP-316
	[Rest API] STP: Configure STP global timer setting by restAPI; system return error and reboot itself.

	2
	ECS4150TIP-315
	[Rest API] voice vlan: DUT not reject to set voice vlan priority to invalid setting value.

	3
	ECS4150TIP-314
	Without a DigiCert certificate, downgrading to specific versions is not allowed.

	4
	ECS4150TIP-313
	[Rest API] lldp: Configure lldp-med-location-civic-device-type to invalid setting by restAPI; DUT not reject it and write incorrect value.

	5
	ECS4150TIP-312
	[Rest API] lldp: Configure lldp-med-location-civic-ca by restAPI; system return error and reboot itself.

	6
	ECS4150TIP-311
	[RestAPI-VoiceVLAN-0010]Voice VLAN OUI Auto Learning failed, port1 not added to VLAN 2 automatically

	7
	ECS4150TIP-309
	[RestAPI-IPv4-SourceGuard-0040] IP Source Guard PUT request returns 400 Bad Request but configuration is successfully applied to the switch.

	8
	ECS4150TIP-307
	After switching EC version to TIP version，Failed to loading the certificates.

	9
	ECS4150TIP-306
	[VoiceVLAN-0460] Voice vlan member port is removed incorrectly when receiving a non-phone LLDP packet from a second neighbor

	10
	ECS4150TIP-305
	【Rest API】support ip http option web/rest-api command

	11
	ECS4150TIP-304
	[Rest API] Support vlan range-start/range-end for interface config.

	12
	ECS4150TIP-303
	input error port number , caused DUT Segmentation Fault

	13
	ECS4150TIP-302
	[LLDP-0140] Executing "show  lldp info remote-device detail ethernet 1/1" causes the CLI to flood with "supported, disabled" messages and freeze.

	14
	ECS4150TIP-301
	Error Handler：show lldp info remote-device detail display errors

	15
	ECS4150TIP-317
	OLS 4.2.0rc1 for Restful API




Runtime V3.2.13.261 Loader V0.0.1.8  OLS 4.2.0rc2
	1
	ECS4150TIP-342
	Merge OLS 4.2.0rc2

	2
	ECS4150TIP-340
	[Rest API] The CLI displays debug messages when ucentral debug is disabled.

	3
	ECS4150TIP-339
	[Rest API] Return correct error messages when adding dhcp relay server failed.

	4
	ECS4150TIP-338
	Configure: The DUT unexpectedly reboots due to a segmentation fault while loading a stacking configuration during system boot.

	5
	ECS4150TIP-334
	NTP: The NTP state becomes incorrect after disabling NTP multiple times.

	6
	ECS4150TIP-331
	Ucaentral client Adapt(UCA) API print some error

	7
	ECS4150TIP-330
	[Rest API] Return error when select-ports of ethernet is invalid

	8
	ECS4150TIP-329
	UcentralRESTAPI: uCentral REST API allows configuring the next hop as 0.0.0.0, but the CLI does not support this configuration.

	9
	ECS4150TIP-319
	[Rest API] should be able to set 0 as voice VLAN ID to disable voice VLAN




Runtime V3.2.14.261 Loader V0.0.1.8  OLS 4.2.0rc3
	1
	ECS4150TIP-350
	Merge OLS 4.2.0rc3

	2
	ECS4150TIP-349
	[REST API] correct mlag-group format

	3
	ECS4150TIP-348
	[Restful API] ECS4150 cannot remove ip-source-guard

	4
	ECS4150TIP-347
	[Rest API] Dot1x multi-auth corresponding to mac-base auth

	5
	ECS4150TIP-346
	[Restful API] ECS4150 cannot remove port-isolation

	6
	ECS4150TIP-345
	[Rest API] Support empty object to set global LLDP default

	7
	ECS4150TIP-344
	[Restful API] failed to delete voice vlan settings




Runtime V3.2.17.261 Loader V0.0.1.8  OLS 4.2.0rc4
	1
	ECS4150TIP-361
	check port is valid of PoE

	2
	ECS4150TIP-360
	Merge OLS 4.2.0rc4

	3
	ECS4150TIP-359
	[REST API] check port is valid of PoE

	4
	ECS4150TIP-358
	[REST API] clear per port ipsg

	5
	ECS4150TIP-357
	[REST API] ACL: ignore match VLAN when match untag packet type

	6
	ECS4150TIP-355
	[REST API] Use 2 pass processing for vlan tag/untag/pvid configurations.

	7
	ECS4150TIP-353
	[REST API] clear port LACP setting

	8
	ECS4150TIP-352
	[REST API] reset storm control; ECS4150TIP-352 [REST API] clear port LACP setting

	9
	ECS4150TIP-351
	[REST API] spanning-tree status workaround

	10
	ECS4150TIP-362
	The ECS4150 crashes when a non-existent port channel is added as a member of an MLAG group.

	11
	ECS4150TIP-356
	Debug DHCP client can not get IP address issue when receiving cloud config




Runtime V3.2.18.261 Loader V0.0.1.8  OLS 4.2.0rc5
	1
	ECS4150TIP-369
	DHCP client issue about get default-router

	2
	ECS4150TIP-368
	Merge OLS uCentral Client 4.2.0rc5

	3
	ECS4150TIP-354
	EC and OLS Version can compatible with each other

	4
	ECS4150TIP-367
	Failed to configure port-channel load-balance using the RESTful API

	5
	ECS4150TIP-363
	Fail to remove voice vlan settings.

	6
	ECS4150TIP-366
	ECS4150 web find a exception

	7
	ECS4150TIP-365
	When switches are reset to default, the backup configuration files should be deleted




Runtime V3.2.19.262 Loader V0.0.1.8  OLS 4.2.0rc5
	1
	ECS4150TIP-387
	when restapi carry unit.password field, it will change the passwod and type instead of using original type

	2
	ECS4150TIP-386
	[RestAPI] fix clear voice vlan oui

	3
	ECS4150TIP-377
	[RestAPI] ethernet clear voice vlan by {}

	4
	ECS4150TIP-375
	when user don't follow schema string type but using integer, it will cause exception

	5
	ECS4150TIP-373
	Add uCentral Client Self-Test commands

	6
	ECS4150TIP-372
	When enabled 802.1x and Mac authentication in PORT, LLDP packets need to be processed first

	7
	ECS4150TIP-370
	POE need read the voltage and current information

	8
	ECS4150TIP-299
	Error Handler：Modify the CGI return value and include the error code value in the JSON message - LLDP MLAG MSTP STP LACP PortTrunk.



Runtime V3.12.22.262 Loader V0.0.1.8  OLS 4.2.0
	1
	ECS4150TIP-406
	Enhance the watchdog and exception log

	2
	ECS4150TIP-405
	[RestAPI] Support pvid tag for interface schema.

	3
	ECS4150TIP-404
	Reload Switch， segmentation fault occured.

	
	ECS4150TIP-401
	The session number incorrectly starts at 4 instead of 1 when connecting to the DUT via SSH or Telnet.(on tip branch)

	
	ECS4150TIP-398
	SSH continuously displays abnormal log messages

	
	ECS4150TIP-396
	UCA library fails to get ethernet info and stats



Runtime V3.12.26.262 Loader V0.0.1.8  OLS 4.2.1rc1
	
	ECS4150TIP-439
	Missing symbolic link of /etc/ucentral in OLS debugging version

	
	ECS4150TIP-436
	ECS4150 phase3 TIP version need support detail DDM info

	
	ECS4150TIP-434
	Merge OLS 4.2.1rc1

	
	ECS4150TIP-430
	[Restful API] Some acl-rules are not bound to selected ports correctly

	
	ECS4150TIP-423
	Add RestAPI function for ASK4.

	
	ECS4150TIP-422
	[Restful API] support ucentral v4.2.1

	
	ECS4150TIP-420
	[Restful API] correct radius server-authentication-port

	
	ECS4150TIP-419
	[Restful API] Unable to set acl-rules

	
	ECS4150TIP-418
	[Restful API] Cannot reset pvid while trying to delete a VLAN

	
	ECS4150TIP-415
	when reset trunk port it fail.

	
	ECS4150TIP-414
	Using  MobaXterm_Personal ssh log in switch,  segmetition fault occurs, and  show log flash  An exception occurs.

	
	ECS4150TIP-486
	ssh connect and exec copy tftp running will cause crash

	
	ECS4150TIP-409
	Merge OLS 4.2.0 with Self-Test




Runtime V3.12.30.263 Loader V0.0.1.8  OLS 4.2.1rc2
	[bookmark: _Hlk235779919]
	ECS4150TIP-467
	[Restful API] Add dhcp relay server not working.

	
	ECS4150TIP-466
	[Rest API] sometimes set NTP multiple times cause exception

	
	ECS4150TIP-463
	Adding/Deleting DHCP Relay Server via CLI unexpectedly clears the Uplink Gateway

	
	ECS4150TIP-461
	Merge OLS 4.2.1rc2 for ECS4150 and ECS5550

	
	ECS4150TIP-460
	DHCP client issue about get default-router

	
	ECS4150TIP-459
	[Rest API] add ethernet dot1x intrusion-action

	
	ECS4150TIP-458
	 [Rest API] enhancement of storm control

	
	ECS4150TIP-450
	[Restful API] redirect v4.2.1 to original version

	
	ECS4150TIP-448
	User root can not login after changing EC version to tip version

	
	ECS4150TIP-443
	[Restful API] Config interfaces[].ipv4.dhcp-snoop-vlan-enable has error messages.

	
	ECS4150TIP-442
	ASK4 need storm-control function support percent

	
	ECS4150EC-1187
	ECS4150 Phase3 TIP support display system temperature via UCA.

	
	ECCLOUD-10004
	 [ASK4_Restful] DNS function is not working properly




Runtime V3.12.31.263 Loader V0.0.1.8  OLS 4.2.1rc2
	
	ECS4150TIP-487
	Fix netcfg_proc SIGSEGV crash and OM semaphore leak causing frequent reboot

	
	ECS4150TIP-485
	[RestAPI] it return ok after input decimal point of service_log

	
	ECS4150TIP-484
	[RestAPI] it return ok after input decimal point of lacp parameters

	
	ECS4150TIP-483
	[RestAPI]it return ok after input any alphabets and special characters of recover-time of loopback-detection

	
	ECS4150TIP-482
	[RestAPI]it should not return OK after setup decimal point of loopback-detection parameters

	
	ECS4150TIP-481
	[RestAPI]it should not return OK after setup decimal point of storm-control parameters

	
	ECS4150TIP-478
	[RestAPI]it should not return OK after setup decimal point of transceiver-threshold parameters

	
	ECS4150TIP-476
	RestAPI (DAI): DUT not reject this DAI rate-limit setting with non-integer value. 

	
	ECS4150TIP-475
	RestAPI (exclude vlan): DUT not reject this exclude vlan-id setting with non-integer value. 

	
	ECS4150TIP-473
	RestAPI (LLDP): DUT not reject this lldp-med-location-civic-ca-type setting with non-integer value.

	
	ECS4150TIP-472
	RestAPI (PoE): DUT not reject this invalid power-limit setting with non-integer value.




Runtime V3.12.32.263 Loader V0.0.1.8  OLS 4.2.1rc2
	
	ECS4150TIP-489
	 [RestAPI] support ethernet speed 0 to enable auto-nego

	
	ECS4150TIP-488
	Default support ZTP for all simba




Runtime V3.12.33.263 Loader V0.0.1.8  OLS 4.2.1rc4
	
	ECS4150TIP-491
	update OLS version to 4.2.1rc4

	
	ECS4150TIP-490
	[RestAPI] set port speed by physical port




[bookmark: _Hlk225252988]OLS Version：

OLS4.2.1rc2
	
	[ECCLOUD-8845]
	[Restful] couldn't use DHCP option 138 URL

	
	ECCLOUD-10018
	[ASK4_Restful] couldn't modify system password



OLS4.2.0
	1
	ECCLOUD-8903
	[Restful] static trunk data of cloud statistic information is not correct

	2
	ECCLOUD-8890
	[Restful] couldnt push default config after getting error code 1

	3
	ECCLOUD-8888
	[Restful] ACL config has fail rate to push

	4
	ECCLOUD-8846
	[Restful] couldn't use Demo insta certificate

	5
	ECCLOUD-8629
	[Restful] couldn't apply guest_vlan config

	6
	ECCLOUD-8218
	[Restful] Configuration persists after removing the corresponding block from JSON input

	7
	ECCLOUD-8199
	[Restful] 4.2.0 Embedded Test Facility



OLS4.2.0rc5
	1
	ECCLOUD-8420
	[Restful API] diagnostic files should contain backup and current configuration files

	2
	ECCLOUD-8421
	[Restful API] When switches are reset to default, the backup configuration files should be deleted

	3
	ECCLOUD-8624
	[Restful] Needs to block DHCP option if the length is over limitation




OLS4.2.0rc4
	1
	ECCLOUD-8034
	[Simba] ucentral-client vulnerable to stack-based buffer overflow via DHCP option

	2
	ECCLOUD-8281
	[OLS] Switch always duplicates log messages

	3
	ECCLOUD-8302
	[Restful API] curl_easy_perform() gets a timeout with long latency request

	4
	ECCLOUD-8283
	[Restful API] There is no RSTP event in console logs

	5
	ECCLOUD-8342
	[Restful] RSTP event is not working

	6
	ECCLOUD-8397
	[Restful API] ucentral-client fails to convert mlag members port name to Simba format



OLS4.2.0rc3
	1
	ECCLOUD-8099
	[RestfulAPI] Can't see uplink interface

	2
	ECCLOUD-8193
	[Restful API] Port isolation is not working on ECS4150 v4.2.0 rc2

	3
	ECCLOUD-8192
	[Restful API] couldn't apply port mirror config to ECS4150 v4.2.0 rc2

	4
	ECCLOUD-8196
	[Restful API] couldn't apply IGMP static group config to ECS4150 v4.2.0 rc2

	5
	ECCLOUD-8095
	[RestfulAPI] Can't use SSB function

	6
	ECCLOUD-8219
	[Restful API] IPSG static binding failed with HTTP 400: Invalid MAC format "58-11-22-E1-B5-29".

	7
	ECCLOUD-8227
	[Restful API] Filter out POE settings on SFP and non-POE Ethernet ports

	8
	ECCLOUD-8034
	[Simba] ucentral-client vulnerable to stack-based buffer overflow via DHCP option



OLS4.2.0rc2
	1
	ECCLOUD-8069 
	[OLS] Push ntp settings cuase ucentral-client crash

	2
	ECCLOUD-8100
	UCA sometimes fails to get state information



OLS4.2.0rc1 
	1
	ECCLOUD-3206
	Support IP Source Guard

	2
	ECCLOUD-3200
	Support Dynamic ARP Inspection

	3
	ECCLOUD-5949
	Support Storm Control

	4
	ECCLOUD-3190
	Support MC-LAG (MLAG)

	5
	ECCLOUD-7829
	Incorrect log reason and blocked-

	6
	ECCLOUD-7843
	refactor state pipeline, add realtime updates, and improve STP stats

	7
	ECCLOUD-7672
	Forbid firmware downgrade without Digicert

	8
	ECCLOUD-7985
	 [OLS] State message enhancement

	9
	[ECCLOUD-7785]
	After upgrading the 4.1.2rc2, it shows error1: upgrade failed

	10
	ECCLOUD-7672
	Forbid firmware downgrade without Digicert




Loader V0.0.0.4
	
	Initial Version




Runtime V1.0.0.1
	
	Initial Version




WORK AS DESIGNED (WAD) EPRS:

KNOWN BUGS AND ISSUES:

Any other problems than those listed above should be reported to our Technical Support Staff.
NA

KNOWN RESTRICITIONS AND LIMITATIONS:

	
	Limitation Type
	Description

	1
	Software limitation
	For verify chip can support full multicast entry. The speed of data/control packet which used for igmp snooping learning shall not in line speed.

	2
	Software limitation
	Web Authentication only support IPv4 HTTP

	3
	Software limitation
	Due to Jquery software limitation. The web browser need IE 9+, Chrome 54+, Firefox 52+ or Opera 41+.

	4
	Software limitation
	Support muintuple vlan tag by software, but have limitation: can not support the packet need linux kernel process, like management features, arp, telnet, ping, tracerout, routing, snmp, ipv6…etc. [ES4627MB-FLF-EC-00889]

	5
	Chip limitation
	ECS4150EC-48 DHCP-Snooping-0340：the rate limit of dhcp snooping does not work well
According to the chip documentation, their speed limit is not 100% accurate, and the speed limit value is calculated by accumulating 10 seconds.

	6
	Chip limitation
	Casued by Phy limit, can not support auto-negotiate of flow-control，We use force mode instead.So if link up with 100M/1G full，flow-control type should always Dot3X，10/100 half type should be backpress.

	7
	Phy chip limitation
	ECS4150EC-63
The link flapping is caused by back-pressure and link would be up after back-pressure condition is gone(This Back-pessure only 100M/10M half on ECS4150-AC5)

	8
	Chip limitation
	ECS4150EC-64
Per system, IC have 1 mirror buffer, after this packet is send out, it can be used for mirroring the next packet again. 
So you can not enable the mirroring, source, destination or multiple at ac5/ac3, ac3bxh solution. 
So when mirror two streams at same time,the mirror packets will loss

	9
	Chip limitation
	After the SFP port is switched to 1G linkup after 10G linkup, if the traffic is blocked and the CLI command “show counter” displays “Internal Mac Transmit Errors / Fragments”, you need to unplug the port module or shutdown/no shutdown port to change the port link status, then the streaming will return to normal (generally, this problem will occur when the device is switched to 1G after the first 10G linkup after startup)

	10
	Chip limitation
	Dynamic QoS Assignment only support configure one acl per port: Marvell support ACL resource are finite, so the upper software limit only support configure one acl per port or per function;when mac-authentication enable Dynamic Qos Assignment base Radius, so also only support configure one acl per port, multiple acls will authentication failure.

	11
	Chip limitation
	AC5X does not support half-duplex

	12
	Software limitation
	cpssDxChMirrorRxPortSet is called to set mirrored port when setting port mirror, and it is also called by sflow-sampling. So you can not set sflow-sampling and mirrored port on the same physical port at the same time.

	13
	Chip limitation
	For AC5X devices, when a SFP interface works on 10G mode and there is streaming on it, and the down/up of the adjacent SFP interfaces will cause packet loss on the streaming interface.

	14
	Chip limitation
	Cable-diag accuracy issues:  For link-down ports, the reported distance to a fault is accurate to within +/- 2 meters. For link-up ports, the accuracy is +/- 10 meters.

	15
	Chip limitation
	For AC5X devices, FDB does not support qos marking, and igmpsnp/mldsnp does not support priority function

	16
	Chip limitation
	For AC5X, can not adapt the media-type of DAC cable(kr) and fiber(sr_lr) automatically for 49-54 ports. So add a CLI command for set it manually :
Vty-1(config-if)#media-type sfp-forced ifmode ?
kr Specifies forced ifmode as KR
sr_lr Specifies forced ifmode as SR_LR
The mode is fiber(sr_lr) by default, so if you need to insert DAC cable on a port, you have to set the mode to kr by this command.


	17
	Chip limitation
	ECS4150EC-377:
On Marverll chips, the output ratelimit is non-coninunous, only a specific set of values can be set. When we set a output ratelimit value, accturely we can only select a nearest value between these specific values.
Because AC5 and AC5X belong to different chips, the set of values all different.
For AC5X, when the value of output ratelimit is small (less than 637), the interval is 25.
75:64-87
100:88-112
125:113-137
150:138-162
175: 163-187
200: 188-212
225: 213-237
And so on
625: 613-637
When the ratelimit output value is larger than 637, the accuracy is within %2

For AC5, test according to the following specifications:
When the value of output ratelimit is small (less than 2055), the interval is 30 or 31.
61: 64-90
91:91-120
121:121-151
152:152-181
182: 182-211
212: 212-241
242:242-271
272:272-302
And so on
When the ratelimit output value is larger than 2055, the accuracy is within %2

	18
	Chip limitation
	ECS4150EC-409:
Marvell currently does not have good support for half-duplex collision counting.






COMPLIANCE SUPPORT:

	Compliance Level
	Compliant

	
	


Known Anomalies: None.


IEEE STANDARDS SUPPORT:

	Standard
	Title

	IEEE 802.1D
	Transparent Bridging Specifications (ISO/IEC 10038)

	IEEE 802.1p
	Traffic Class Expediting and Dynamic Multicast Filtering

	IEEE 802.1Q
	Virtual Bridged Local Area Networks

	IEEE 802.1w
	Rapid Spanning Tree

	IEEE 802.2    
	Local Area Networks, Logical Link Control (LLC)

	IEEE 802.3    
	CSMA/CD 9 (ISO/IEC 8802-3)

	IEEE 802.3I   
	10Base-T (ISO/IEC 8802-3, clause 14)

	IEEE 802.3u  
	100Base-TX (ISO/IEC 8802-3, clause 25)

	IEEE 802.3x
	Flow Control

	IEEE 802.3z
	1000Base-SX, 1000Base-LX

	IEEE 802.3ab
	1000Base-TX

	IEEE 802.3ac
	VLAN Tag

	IEEE 802.3ad
	Link Aggregation

	IEEE 802.1X
	Port-based Network Access Control




IETF STANDARDS MIB SUPPORT:
	RFC No.
	Title
	Groups Supported

	1907
	SNMPv2-MIB (MIB II)
	- system group ( 1-9)
- snmp group (1-6, 8-22, 24-32)

	2011
	IP-MIB (MIB-II)
	- ip group (1-20, 22-23)
- icmp group (1-26)

	2012
	TCP-MIB (MIB-II)
	- tcp group (1-15)(tcpConnTable only support read.)

	2013
	UDP-MIB (MIB-II)
	- udp group (1-5)

	IEEE
802.1X MIB
	IEEE8021-PAE-MIB
	- dot1xPaeSystem (1-2)
- dot1xPaeAuthenticator (1-3)(not support per-port timer setting)

	1493
	Bridge MIB
	- dot1dBase group (1-4)
- dot1dStp group (1-15)
- dot1dTp group (1-4)
- dot1dStatic group (1)

	2863
	Interfaces Evolution MIB (IF-MIB)

	- interface group (1-2) (ifadminStatus not support set to  3(testing))
- ifXTable group (1)
- ifStackTable group (1)(support   
read-only)

	2819
	 RMON MIB
	- statistics group (1)
- history group (1-2)
- alarm group (1)
- event group (1-2)

	2618
	RADIUS MIB
	- radiusAuthClientMIB (1)

	2665
	Etherlike MIB
	- dot3StatsTable group (1-19)

	2737
	Entity MIB
	· entityPhysical group (1-16) 
(support read-only)

	2674
	P-bridge
	- dot1dExtBase group (1-4)
- dot1dPriority group (1,3) 
- dot1dGarp group (1)

	2674
	Q-bridge
	- dot1qBase group (1-5)
- dot1qTp group (1-2)
- dot1qStatic group(1)
- dot1qVlan (1-5) (9-10)

	V-Bridge MIB
	V-Bridge MIB
	- dot1vProtocol group

	3636
	MAU MIB
	· dot3IfMauBasicGroup
· dot3IfMauAutoNegGroup



	1612
	DNS Reslover MIB
	· dnsServConfig
· dnsServCounter
· dnsServCounterAuthAns
· dnsServCounterAuthNoNames
· dnsServCounterAuthNoDataResps
· dnsServCounterNonAuthDatas
· dnsServCounterNonAuthNoDatas
· dnsServCounterReferrals
· dnsServCounterErrors
· dnsServCounterRelNames
· dnsServCounterReqRefusals
· dnsServCounterReqUnparses
· dnsServCounterOtherErrors
· dnsServOptCounter
· dnsResMIBObjects
· dnsResConfig
· dnsResCounter
· dnsResCache
· dnsResCacheStatus
· dnsResCacheMaxTTL
· dnsResCacheGoodCaches
· dnsResCacheBadCaches
· dnsResOptCounter

	3411
	SNMP FrameWork
	· snmpFrameworkMIBObjects

	3412

	SNMP MPD MIB
	· snmpMPDMIBObjects

	3413
	SNMP Target MIB
	· snmpTargetObjects

	3413

	SNMP Notify MIB
	· SnmpNotifyObjects
· snmpNotifyTable
· usmMIBObjects

	3415
	SNMP View-Based ACM MIB
	· vacmMIBObjects
· Private MIB
· switchMgt
· portMgt
· trunkMgt
· lacpMgt
· staMgt
· tftpMgt
· restartMgt
· mirrorMgt
· igmpSnoopMgt
· ipMgt
· bcastStormMgt
· vlanMgt
· priorityMgt
· trapDestMgt
· qosMgt
· securityMgt
· sysLogMgt
· lineMgt




ECS4150 SERIES PRIVATE ENTERPRISE MIB SUPPORT:

	Title
	Version

	ECS4150.mib
	202104080000Z




SNMP TRAP SUPPORT:
	RFC No.
	Title

	RFC 1215
	ColdStart (v1)
warmStart (v1)
linkDown  (v1)
linkUp    (v1)
authenticationFailure (v1)

	RFC 1907
	coldStart (v2c)
warmStart (v2c)
authenticationFailure (v2c)

	RFC 2863
	linkDown  (v2c)
linkUp    (v2c)

	RFC 1493
	newRoot (v1)
topologyChange (v1)

	RFC 1757
	risingAlarm (v1)
fallingAlarm (v1)

	RFC 2819
	risingAlarm (v2c)
fallingAlarm (v2c)




Customer Support:

By Phone:
By Email: 
By Web:
       By Fax:
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