

		
ENGINEERING RELEASE NOTES

Gigabit Ethernet Switch ECS5500-12T/12P
Phase 1 Firmware Version 1.1.9.262


INTRODUCTION:
[bookmark: OLE_LINK26][bookmark: OLE_LINK29]The ECS5500-12T/12P is a 8*100/1000/1G/2.5G/5G/10G Base-T ports and 2*10G SFP and 2*10G BASE-T uplink ports L2+ Switch.

[bookmark: OLE_LINK30]Local Console Management (LCM) allows the user to monitor and configure the ECS5500 Series from a VT-type terminal. LCM can be used to configure features such as SNMP community names and access rights, Port Enable/Disable, firmare downloads, and Device IP address as well as most other parameters. LCM can also provide statistical and diagnostic information about the entire device or an individual port.

[bookmark: OLE_LINK8]Management of the switch is password protected; the same password is used for LCM and for the Web browser interface. Prior to accessing the Management Module via a network connection, a valid IP address, subnet mask, and in some cases a default gateway must be configured using an out-of-band connection or the DHCP protocol. The management option provides SNMP, RMON (4 groups: 1,2,3,9), and Web management for system control and statistical monitoring.


	It is recommended that one thoroughly review this release notes prior to the installation or upgrade of this product.



FIRMWARE SPECIFICATION:

	Status
	Version No.
	Type
	Release Date

	Phase1 NTC Testing Version
	1.1.9.262
	EIT and NTC Test version
Gitlab: rtk_main 
	2026/6/25

	Phase1 NTC Testing Version
	1.1.8.253
	EIT and NTC Test version
Gitlab: rtk_main 
	2025/8/3

	Phase1 EIT&NTC Testing Version
	1.1.7.253
	EIT and NTC Test version
Gitlab: rtk_main 
	2025/7/11

	Phase1 NTC Testing Version
	1.1.6.252
	NTC Test version
Gitlab: rtk_main
	2025/4/2

	Phase1 EIT & NTC Testing Version
	1.1.5.251
	EIT and NTC Test version
Gitlab: rtk_main
	2025/3/21

	Phase1 NTC Testing Version
	1.1.4.251
	NTC Test Version
Gitlab: rtk_main
	2025/3/7

	Phase1 EIT Testing Version
	1.1.3.251
	EIT Test version
Gitlab: rtk_main
	2025/2/24

	Phase1 NTC Testing Version
	1.1.2.244
	NTC Test version
Gitlab: rtk_main 
	2024/12/27

	Phase1 EIT Testing Version
	1.1.1.243
	EIT Test version
Gitlab: rtk_main
	2024/9/9

	[bookmark: OLE_LINK31][bookmark: OLE_LINK1]Phase1 EIT Testing Version
	1.1.0.243
	[bookmark: OLE_LINK3]EIT Test version
Gitlab: rtk_main
	2024/9/3


LOADER:

	Status
	Version No.
	Type
	Release Date

	Test Version
	0.0.2.3
	Gitlab: rtk_main Branch 
	2024/9/9

	Test Version
	0.0.2.4
	Gitlab: rtk_main Branch
	2024/12/27

	Test Version
	0.0.2.5
	Gitlab: rtk_main Branch 
	2025/2/24

	Test Version
	0.0.2.6
	Gitlab: rtk_main Branch
	2025/3/7

	Test Version
	0.0.2.7
	Gitlab: rtk_main Branch
	2025/7/11



DIAG IMAGE:

	Status
	Version No.
	Type
	Release Date

	Test Version
	
	Diag image
	



HARDWARE COMPATIBILITY:	

ALL


BOOTPROM COMPATIBILITY:

ALL


NETWORK MANAGEMENT SOFTWARE SUPPORT:

	NMS Platform
	Version No.
	Module No.

	TBD
	 
	 



If you install this image, you may not have control of all of the latest features of this product until the next version(s) of network management software. Please review the software release notes for your specific network management platform for details.


SUPPORTED FUNCTIONALITY:


INSTALLATION AND CONFIGURATION NOTES:

[bookmark: OLE_LINK34][bookmark: OLE_LINK33]In general, the ECS5500 Series Switch will be shipped to you pre-configured with this version of firmware. If you would like to upgrade an existing ECS5500 Series Switch, please follow the TFTP download instructions that are included with your firmware image upgrade kit.
 
FIRMWARE CHANGES AND ENHANCEMENTS:

The following Known Issues have been fixed in this release of firmware.
Runtime V1.1.9.262 Loader V0.0.2.7
	
	ECS5500EC-266
	9b3a84a
	Upgrade OpenSSH from 9.8p1 to 10.3p1

	
	ECS5500EC-264
	66eebca2
	The session number incorrectly starts at 4 instead of 1 when connecting to the DUT via SSH or Telnet.(on phase1 branch)



Runtime V1.1.8.253 Loader V0.0.2.7
	
	ECS5500EC-239
	68c8c10
	mgmtd upgrade to V1.9.12-17625

	
	ECS5500EC-232
	c059552
	CableDiag: The type status is incorrect when the UTP port is open (break).

	
	ECS5500EC-233
	7fdfb01
	CableDiag: The connection status of cable-diagnostics always shows N/A and does not reflect the actual connection state.

	
	ECS5500EC-225
	1915925
	ECS5500 support usb file command



Runtime V1.1.7.253 Loader V0.0.2.7
	
	ECS5500EC-205
	68c8c10
	Without backdoor - MD5 Checksum File Generation.

	
	ECS5500EC-215
	c059552
	Create VLAN will cause the configuration to fail when trunk ID is 27, 28

	
	ECS5500EC-184
	7fdfb01
	NTP: The DUT will freezing and reboot when added and delete the ntp server more times.

	
	ECCLOUD-5468
	a0fa418
	After downgrade device cannot register to the Cloud.

	
	ECS5500EC-221
	a9a4f64
	upgrade SDK to V4.0.4 patch578

	
	ECCLOUD-5799
	6f59c07
	Add adoptd_private functionality.

	
	ECS5500EC-222
	e2f5aae
	ECS5500 add TIP PBE

	
	ECS5500EC-228
	d337578
	Switch will print error message like “/etc/rc: /etc/rc.accton: line 5: busybox true: not found“ when startup

	
	ECS5500EC-227
	d942da8
	nokia enhancment: record the operation from web into log

	
	ECS5500EC-226
	d942da8
	It is need logged if the maximum number of login attempts is exceeded

	
	ECS5500EC-140
	a9a4f64
	Cable Diagnostics: The function doesn't work compare behavior

	
	ECS5500EC-168
	a9a4f64
	Sometimes, the some copper port is linkup to 5G after re-plug power cable and then system boot up.





Runtime V1.1.6.252 Loader V0.0.2.6
	
	ECS5500EC-195
	c9116ec
	Without backdoor - Modified version name.

	
	ECS5500EC-198
	60cc8a0
	Cppcheck find memory leak issue.

	
	ECS5500EC-81
	68c8c10
	ACL: CLI cannot set a MAC ACL with the IP option.

	
	ECS5500EC-197
	b26bafe
	Add mgmtd with ECS5500 series support

	
	ECS5500EC-201
	466260b
	remove the default snmp community （public and private）

	
	ECS5500EC-169
	20904c2
	The port utilization in 2.5G speed always show 100%




Runtime V1.1.5.251 Loader V0.0.2.6
	1
	ECS5500EC-159
	3ddcd96
	DDM SYSLOG: The alarm and warning log is incomplete(suggest add threshold is xxx dBm and current is xxx dBm display)

	
	ECS5500EC-183
	8aef2e0
	LACP: The DUT will display a debug message when LACP is enabled, and the configuration is saved or displayed using the show running-config command.

	
	ECS5500EC-178
	b425c1e
	IPv6 Source Guard: Failed to replaced this dynamic IPv6 SG entries to static binding.

	
	ECS5500EC-158
	c435723
	The WebUI cannot display hardware counter information of IP/IPv6 ACL.

	
	ECS5500EC-190
	8beb118
	System Test: The image will disappear when power off/on the DUT.

	
	ECS5500EC-191
	8beb118
	System Test The license will disappear when power off/on.


	
	ECS5500EC-194
	8beb118
	ProtocolVlan: The DUT will pop worng message when add the protocol-vlan entries





Runtime V1.1.4.251 Loader V0.0.2.6
	1
	ECS5500EC-152
	8b924b0
	IPv6 Source Guard: Enable IPv6 Source Guard, DHCPv6-snp and nd-snooping at same time; DUT cannot drop invalid IPV6 packets.

	
	ECS5500EC-167
	01f6d1d
	UDLD: No notification for udld Link Detectio trap.

	
	ECS5500EC-73
	c63656a
	remove recovery partition from SPI NAND Flash

	
	ECS5500EC-94
	874d2a9
	MIB: The mib fie is miss option by "fileAutoUpgradeMgt"

	
	ECS5500EC-145
	172eac6
	DiffServ: The webUI has unsupported policy configurations.

	
	ECS5500EC-134
	910f799
	Voice VLAN: DUT not reject to change switch port mode to Access as enable auto mode on Port.

	
	ECS5500EC-122
	ea9ab96
	[Enhancement] Web-Auto Upgrade: It should be add option by "Automatic Opcode Upgrade Reload"

	
	ECS5500EC-176
	a49d4e0
	Configure alias name cause CLI task crash

	
	ECS5500EC-165
	18e602b
	The official build of 248 day LLDP issue patch

	
	ECS5500EC-112
	18e602b
	unit of measure using wrong unit.

	
	ECS5500EC-98
	c486b51
	IPv6-AddrConfig: The value of ND reachable time would return to the default value after setting to 0 and rebooting.

	
	ECS5500EC-156
	22b12f7
	MVR6: Robustness behaviour is incorrect after saving and restarting.




Runtime V1.1.3.251 Loader V0.0.2.5
	1
	ECS5500EC-74
	1ad51a7
	add recovery mechanism when pressing ctrl+r in uboot

	
	ECS5500EC-99
	05764e8
	ERPS: After we inject CDP frames; this data looping occurs between 2 DUT.

	
	ECS5500EC-83
	747438a
	Static route: DUT doesn't display default route with specific sub-mask 31

	
	ECS5500EC-94
	16aba97
	IPv6-AddrConfig: DUT doesn't support 1/127 prefix.

	
	ECS5500EC-108
	a7e0f63
	MVR: Multicast data groups cannot be cleared the by clear command.

	
	ECS5500EC-92
	0a7214d
	IPv6-MLD-SNP: Dynamic group entries cannot be deleted when add and remove static mrouter port.

	
	ECS5500EC-93
	cd85ed4
	IPv6-MLD-SNP: DUT doesn't forward the report to mrouter port when enable querier and proxy-reporting.

	
	ECS5500EC-109
	5cc9527
	MVR: The uptime of unregistered groups count.

	
	ECS5500EC-115
	0c00de1
	MVR6 VLAN can be overlapped.

	
	ECS5500EC-110
	787106d
	MVR: All vlans would be considered DVLAN in mvr statistics input.

	
	ECS5500EC-86
	3506294
	CLI: no capabilities 10half/10full is in running-config  and startup-config by default

	
	ECS5500EC-119
	c7224d5
	add updt command to update u-boot.bix in uboot

	
	ECS5500EC-102
	6097d64
	IPv6-AddrConfig: The prefix length prompt message is incorrect in the ipv6 nd prefix command.

	
	ECS5500EC-101
	0c0de98
	IPv6-AddrConfig: The RA sent by the DUT doesn't contain prefix information of the VLAN IP address.

	
	ECS5500EC-127
	1645931
	TWAMP: CLI shows wrong format when the address is long IPv6 addres

	
	ECS5500EC-85
	f161648
	AMTR: After we save and rebooting this DUT; it lose this static mac-address of LACP trunk.

	
	ECS5500EC-148
	f161648
	LACP: Create static mac-address that will disappear after save and reboot.

	
	ECS5500EC-142
	45e468b
	MVR6: G Query cannot count on the receiver ports.

	
	ECS5500EC-143
	d9e4cd3
	MVR6:mvr6 port type can be set to recevier port when port mode is access.

	
	ECS5500EC-26
	b5c4046
	Enhance the command "show tech-support" that the result needs to include all what can the user show into it

	
	ECS5500EC-104
	b5c4046
	Copy File: Failed to copy log to TFTP server.

	
	ECS5500EC-89
	fa387f8
	PPoE-IA: The PPPoE-IA configuration will disappear when save and reboot.

	
	ECS5500EC-132
	19042cf
	UserAuth-Local: DUT not record this password changing log as modify user password.

	
	ECS5500EC-121
	4f0bbb6
	SNTP Client: The SNTP can't set ipv6 address

	
	ECS5500EC-130
	4c25473
	Irregular Operation: DUT can reload when firmware transmission(issue of sequence)

	
	ECS5500EC-135
	c777a8b
	SFTP_FTP_TFTP: The copy sftp/ftp/tftp add-to-running-config success, but log is not recorded.

	
	ECS5500EC-150
	3202ee4
	MVR6: The behavior differs from ECS4655 when the normal port, which is an MVR6 VLAN member, receives the join report.

	
	ECS5500EC-151
	3202ee4
	MVR6: The behavior differs from ECS4655 when the inactive receiver port, which is an MVR6 VLAN member, receives the join report.

	
	ECS5500EC-68
	4dfa8e3
	[IPv4-RemotePing-0100, 0110] MAXSIZE_pingPacketSize is different mibx.json

	
	ECS5500EC-69
	4dfa8e3
	[VLAN-MAC-Based-0060] MAX MAC VLAN Entry is different mibx.json

	
	ECS5500EC-123
	539b873
	MIB: The mib fie is miss option by "fileAutoUpgradeMgt"

	
	ECS5500EC-136
	adf5c7a
	Copy Direction: DUT can accept non-real cfg and other file name then also can set to startup.

	
	ECS5500EC-125
	423b65f
	Web-File: FTP download(opcode or config file) show "Data is invalid" when first to do it.

	
	ECS5500EC-126
	423b65f
	ConfigFileMgmt: DUT cannot copy file to FTP via WebUI after copying file to FTP via CLI.

	
	ECS5500EC-161
	d29ac4f
	design ECS5500 thermal plan

	
	ECS5500EC-147
	488b67f
	IPv6 Source Guard: After we save running setting and rebooting this DUT; it loses all static binding entries.

	
	ECS5500EC-163
	5a9265d
	LACP: The description of Port will change when join in the port-channel or save and reboot.

	
	ECS5500EC-153
	1affc08
	Selective QinQ: Selective QinQ enteris will disappear when join the the member of port-channel interface.

	
	ECS5500EC-149
	491b2fe
	VLAN-Translation: The translation setting can't join to port channel.
Note: The VLAN translation configuration method has been updated to be mutually exclusive between normal ports and trunk ID-based configurations.

	
	ECS5500EC-146
	ea31bf7
	The source IPv6 address is incorrect when the DUT receives other queries.

	
	ECS5500EC-158
	8ef3fdd
	ACL: The WebUI cannot display hardware counter information of IP/IPv6 ACL.

	
	ECS5500EC-100
	8ef3fdd
	SelectiveQinQ: The configure will extra zero when create selective QinQ on CLI and Mib.

	
	ECS5500EC-139
	f81ad77
	WEB: Loopback-detection action miss the option of bcast-discard and port-disable.

	
	ECS5500EC-138
	650bac1
	DHCPv6 Relay: DUT not reject to configure itself as Relay server.

	
	ECS5500EC-131
	3c60647
	PoE: Port1 cannot supply power and the power inline status is incorrect.

	
	ECS5500EC-116
	ae4c45d
	openssl/openssh upgrade

	
	ECS5500EC-90
	ae4c45d
	HTTP-HTTPS: Unable to access the DUT via HTTPS session




Runtime V1.1.2.243 Loader V0.0.2.24
	1
	ECS5500EC-59
	29e113a
	[STP-0670] "Oper Link Type" should be "Point-to-point" when port link with full-duplex.

	
	ECS5500EC-25
	f28343c
	Enhance the extended HTTP/HTTPS/SSH timeout logout time

	
	ECS5500EC-60
	f3973ad
	[SystemBoot] Got "Reset system error" after "copy file running" is executed

	
	ECS5500EC-70
	756e4ff
	Update profile license feature by latest specs

	
	ECS5500EC-71
	6f4ce8f
	Add TIP compatiblity for EC

	
	ECS5500EC-78
	8bd35b5
	support 5500 12T/12P web ui port panel

	
	ECS5500EC-51
	509500f
	design NAND flash layout to store runtime and config

	
	ECS5500EC-80  
	924c721
	modify the oid of 5500



Runtime V1.1.1.243 Loader V0.0.2.3
	1
	ECS5500EC-56
	fcc7d10
	ECS5500 CLI usually fails to ping

	
	ECS5500EC-55
	17a138f
	set RST0 as high to reset both of PCA9543 for HW R0B




Runtime V1.1.0.243 Loader V0.0.2.3
	1
	ECS5500EC-53
	24210d9
	ECS5500 phase1 poe function debug

	
	ECS5500EC-52
	1719e64
	mac-vlan:The 11 and 12 ports of the MAC VLAN cannot be Enable

	
	ECS5500EC-50
	ff63619
	verify and debug powersave

	
	ECS5500EC-48
	19ff233
	Enhance the command "port-utilization" on global config.

	
	ECS5500EC-43
	
	IPv6 srcguard enabled, when adding a static binding entry, all IPv6 packets can go through the port.

	
	ECS5500EC-44
	4ab464c
	verify and debug LED

	
	ECS5500EC-37
	b96fdf
	ECS5500 GPIO/RX_LOS/TX_Disable verify and debug

	
	ECS5500EC-41
	431ba83
	the default STP path cost is different with other brands and spec.

	
	ECS5500EC-39
	61c9027
	The default vlan with MVR is not same  spec defines.

	
	ECS5500EC-15
	2d9b7a2
	Enhance DHCP option 82 setting remote ID from global mode to port interface.

	
	ECS5500EC-22
	4bbd0d3
	ECS5500EC-22 LACP: The ports of 5G cannot form LACP.

	
	ECS5500EC-35
	3c7a126
	ECS5500EC-35 VLAN: Re-enable ipv6 on VLANs, CLI print error message.

	
	ECS5500EC-34
	41d9e59
	CableDiag verify and debug

	
	ECS5500EC-18
	b976577
	debug ECS5500 I2C

	
	ECS5500EC-16
	1e3fc4a
	Need to register all tasks and threads to watchdog

	
	ECS5500EC-32
	2d683e4
	rtk sdk cli can not query ipmcast and mcast hw entry.

	
	ECS5500EC-14
	bc9fbf3
	debug ECS5500 port link



MODIFICATIONS:

WORK AS DESIGNED (WAD) EPRS:
	
	ECS5500EC-165
	WAD
	PoE: Only one port can supply power if we change the power mainpower maximum allocation.

	
	ECS5500EC-155
	WAD
	Selective QinQ: Selective QinQ enteris of LACP will disappear when save and reboot.

	
	ECS5500EC-141
	WAD
	Loopback-detection: The recover time is incorrect from IXIA send LBD packet.

	
	ECS5500EC-133
	WAD
	PoE: Only one port can supply power if we change the power mainpower maximum allocation.

	
	ECS5500EC-103
	WAD
	ERPS: DUT cannot learn maximum VLAN mac addresses.

	
	ECS5500EC-91
	WAD
	IPv6-MLD-SNP: DUT sends the report immediately if the proxy-reporting was enabled and received a general query.

	
	ECS5500EC-88
	WAD
	CLI: The behavior of no ip default-gateway is wrong when adding default gateway via ip default-gateway and ip route command.

	
	ECS5500EC-154
	WAD
	MVR6: The DUT cannot forward the query received from the source port to other source ports.

	
	ECS5500EC-106
	WAD
	Sflow: The Polling Interval is incorrect.



KNOWN BUGS AND ISSUES:
	
	ECS5500EC-82
	ACL: All ports cannot forward packets when binding the IPv6 ACL to a port egress.
	EIT



Any other problems than those listed above should be reported to our Technical Support Staff.
NA

KNOWN RESTRICITIONS AND LIMITATIONS:

	
	Limitation Type
	Description

	3
	Chip limitation
	ECS5500 Port 1-10 does not support forced 1000m, but only forced 100m

	4
	Chip limitation
	RTL9310 chip does not support enabling auto negotiation for fiber port 11/12

	6
	Chip limitation
	RTL9310 chip known issue: sFlow packet won’t be dropped until packet buffer is used out.

	7
	Chip limitation
	CableDiag: Cable length tolerance exceed 10 meters when length less than 10M

	8
	Chip limitation
	TRL9310 chip did not transmit udp packets with sourceport/destination port 0

	9
	Chip limitation
	ACL no discards source MAC with ARP request(because of system will apply an acl to trap arp request packet to cpu,and the priority is hight than the mac acl)

	10
	Chip limitation
	239.x.x.x 224.0.0.x 224.0.1.x these multicast management packets cannot be considered as an unknown packets，and will be flood

	11
	Chip limitation
	Cable test should use cat6a cable,and disable the POE function when testing





COMPLIANCE SUPPORT:

	Compliance Level
	Compliant

	
	


Known Anomalies: None.


IEEE STANDARDS SUPPORT:

	Standard
	Title

	IEEE 802.1D
	Transparent Bridging Specifications (ISO/IEC 10038)

	IEEE 802.1p
	Traffic Class Expediting and Dynamic Multicast Filtering

	IEEE 802.1Q
	Virtual Bridged Local Area Networks

	IEEE 802.1w
	Rapid Spanning Tree

	IEEE 802.2    
	Local Area Networks, Logical Link Control (LLC)

	IEEE 802.3    
	CSMA/CD 9 (ISO/IEC 8802-3)

	IEEE 802.3I   
	10Base-T (ISO/IEC 8802-3, clause 14)

	IEEE 802.3u  
	100Base-TX (ISO/IEC 8802-3, clause 25)

	IEEE 802.3x
	Flow Control

	IEEE 802.3z
	1000Base-SX, 1000Base-LX

	IEEE 802.3ab
	1000Base-TX

	IEEE 802.3ac
	VLAN Tag

	IEEE 802.3ad
	Link Aggregation

	IEEE 802.1X
	Port-based Network Access Control




IETF STANDARDS MIB SUPPORT:
	RFC No.
	Title
	Groups Supported

	1907
	SNMPv2-MIB (MIB II)
	- system group ( 1-9)
- snmp group (1-6, 8-22, 24-32)

	2011
	IP-MIB (MIB-II)
	- ip group (1-20, 22-23)
- icmp group (1-26)

	2096
	IP FORWARD(MIB-II)
	-ipForwardNumber (1)
- ipCidrRouteNumber (3)
- ipCidrRouteNumber (4)

	2012
	TCP-MIB (MIB-II)
	- tcp group (1-15)(tcpConnTable only support read.)

	2013
	UDP-MIB (MIB-II)
	- udp group (1-5)

	IEEE
802.1X MIB
	IEEE8021-PAE-MIB
	- dot1xPaeSystem (1-2)
- dot1xPaeAuthenticator (1-3)(not support per-port timer setting)

	1493
	Bridge MIB
	- dot1dBase group (1-4)
- dot1dStp group (1-15)
- dot1dTp group (1-4)
- dot1dStatic group (1)

	2863
	Interfaces Evolution MIB (IF-MIB)

	- interface group (1-2) (ifadminStatus not support set to  3(testing))
- ifXTable group (1)
- ifStackTable group (1)(support   
read-only)

	2819
	 RMON MIB
	- statistics group (1)
- history group (1-2)
- alarm group (1)
- event group (1-2)

	2021
	RMON2-MIB
	probeCapabilities (probeConfig 1)
probeSoftwareRev (probeConfig 2) probeHardwareRev (probeConfig 3) probeDateTime (probeConfig 4) probeResetControl (probeConfig 5) probeDownloadFile (probeConfig 6) probeDownloadTFTPServer (probeConfig 7) 
probeDownloadAction (probeConfig 8)
probeDownloadStatus (probeConfig 9)

	2618
	RADIUS MIB
	- radiusAuthClientMIB (1)

	2665
	Etherlike MIB
	- dot3StatsTable group (1-19)

	2737
	Entity MIB
	· entityPhysical group (1-16) 
(support read-only)

	2674
	P-bridge
	- dot1dExtBase group (1-4)
- dot1dPriority group (1,3) 
- dot1dGarp group (1)

	2925
	DISMAN-PING-MIB
	pingCtlTable (2)/pingCtlEntry
pingResultsTable (3)/pingResultsEntry pingProbeHistoryTable (4)/pingProbeHistoryEntry
traceRouteCtlTable


	2925
	
DISMAN-TRACEROUTE-MIB
	-traceRouteCtlTable(2)
- traceRouteResultsTable(3)	
- traceRouteProbeHistoryTable(4)
- traceRouteHopsTable(5)

	V-Bridge MIB
	V-Bridge MIB
	- dot1vProtocol group

	3636
	MAU MIB
	· dot3IfMauBasicGroup
· dot3IfMauAutoNegGroup



	1612
	DNS Reslover MIB
	· dnsServConfig
· dnsServCounter
· dnsServCounterAuthAns
· dnsServCounterAuthNoNames
· dnsServCounterAuthNoDataResps
· dnsServCounterNonAuthDatas
· dnsServCounterNonAuthNoDatas
· dnsServCounterReferrals
· dnsServCounterErrors
· dnsServCounterRelNames
· dnsServCounterReqRefusals
· dnsServCounterReqUnparses
· dnsServCounterOtherErrors
· dnsServOptCounter
· dnsResMIBObjects
· dnsResConfig
· dnsResCounter
· dnsResCache
· dnsResCacheStatus
· dnsResCacheMaxTTL
· dnsResCacheGoodCaches
· dnsResCacheBadCaches
· dnsResOptCounter

	3411
	SNMP FrameWork
	· snmpFrameworkMIBObjects

	3412

	SNMP MPD MIB
	· snmpMPDMIBObjects

	3413
	SNMP Target MIB
	· snmpTargetObjects

	3413

	SNMP Notify MIB
	· SnmpNotifyObjects
· snmpNotifyTable
· usmMIBObjects

	3415
	SNMP View-Based ACM MIB
	· vacmMIBObjects
· Private MIB
· switchMgt
· portMgt
· trunkMgt
· lacpMgt
· staMgt
· tftpMgt
· restartMgt
· mirrorMgt
· igmpSnoopMgt
· ipMgt
· bcastStormMgt
· vlanMgt
· priorityMgt
· trapDestMgt
· qosMgt
· securityMgt
· sysLogMgt
· lineMgt




ECS5500 SERIES PRIVATE ENTERPRISE MIB SUPPORT:

	Title
	Version

	ECS5500-Series.mib
	2025030520000Z




SNMP TRAP SUPPORT:
	RFC No.
	Title

	RFC 1215
	ColdStart (v1)
warmStart (v1)
linkDown  (v1)
linkUp    (v1)
authenticationFailure (v1)

	RFC 1907
	coldStart (v2c)
warmStart (v2c)
authenticationFailure (v2c)

	RFC 2863
	linkDown  (v2c)
linkUp    (v2c)

	RFC 1493
	newRoot (v1)
topologyChange (v1)

	RFC 1757
	risingAlarm (v1)
fallingAlarm (v1)

	RFC 2819
	risingAlarm (v2c)
fallingAlarm (v2c)
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